(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LAN7800-I-VSX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LAN7800-I-VSX"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LAN7800-I-VSX"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/268/LAN7800_Data_Sheet_DS00001992H-2891610.pdf"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface IC USB3.1 Gen1 to 10/100/1000 Ethernet Bridge, Industrial temp."
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LAN7800-I/VSX"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, ETHERNET, PHY, USB, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LAN7800-I-VSX_1_1"
				(text "CRYSTAL"
					(at 12.7 -64.77 900)
				)
				(text "USB 3.0"
					(at 17.78 -40.64 900)
				)
				(text "ETH"
					(at 21.59 -38.1 900)
				)
				(text "EEPROM"
					(at 25.4 -64.77 900)
				)
				(pin passive line
					(at 35.56 -22.86 180)
					(length 2.54)
					(name "TRO_P")
					(number "1")
				)
				(pin passive line
					(at 35.56 -25.4 180)
					(length 2.54)
					(name "TRO_N")
					(number "2")
				)
				(pin passive line
					(at 35.56 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "VDD25A")
					(number "3")
				)
				(pin passive line
					(at 35.56 -30.48 180)
					(length 2.54)
					(name "TR1_P")
					(number "4")
				)
				(pin passive line
					(at 35.56 -33.02 180)
					(length 2.54)
					(name "TR1_N")
					(number "5")
				)
				(pin passive line
					(at 35.56 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "VDD25A")
					(number "6")
				)
				(pin passive line
					(at 35.56 -38.1 180)
					(length 2.54)
					(name "TR2_P")
					(number "7")
				)
				(pin passive line
					(at 35.56 -40.64 180)
					(length 2.54)
					(name "TR2_N")
					(number "8")
				)
				(pin passive line
					(at 35.56 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "VDD25A")
					(number "9")
				)
				(pin passive line
					(at 35.56 -45.72 180)
					(length 2.54)
					(name "TR3_P")
					(number "10")
				)
				(pin passive line
					(at 35.56 -48.26 180)
					(length 2.54)
					(name "TR3_N")
					(number "11")
				)
				(pin passive line
					(at 35.56 -15.24 180)
					(length 2.54)
					(name "VDD25A")
					(number "12")
				)
				(pin passive line
					(at 35.56 -7.62 180)
					(length 2.54)
					(name "VDD12_SW_OUT")
					(number "13")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD_SW_IN")
					(number "14")
				)
				(pin passive line
					(at 35.56 -10.16 180)
					(length 2.54)
					(name "VDD12_SW_FB")
					(number "15")
				)
				(pin passive line
					(at 35.56 -58.42 180)
					(length 2.54)
					(name "EECS")
					(number "16")
				)
				(pin passive line
					(at 35.56 -66.04 180)
					(length 2.54)
					(name "EEDI")
					(number "17")
				)
				(pin passive line
					(at 35.56 -63.5 180)
					(length 2.54)
					(name "EEDO")
					(number "18")
				)
				(pin passive line
					(at 35.56 -60.96 180)
					(length 2.54)
					(name "EECLK")
					(number "19")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDVARIO")
					(number "20")
				)
				(pin passive line
					(at 35.56 0 180)
					(length 2.54)
					(name "VDD12CORE")
					(number "21")
				)
				(pin passive line
					(at 35.56 -73.66 180)
					(length 2.54)
					(name "~{PME}")
					(number "22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "VBUS_DET")
					(number "23")
				)
				(pin passive line
					(at 35.56 -71.12 180)
					(length 2.54)
					(name "~{SUSPEND}")
					(number "24")
				)
				(pin passive line
					(at 35.56 -2.54 180)
					(length 2.54)
					(name "VDD12A")
					(number "25")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "USB2_D_P")
					(number "26")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "USB2_D_N")
					(number "27")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "USB3_TXD_P")
					(number "28")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "USB3_TXD_N")
					(number "29")
				)
				(pin passive line
					(at 35.56 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VDD12A")
					(number "30")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "USB3_RXD_P")
					(number "31")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "USB3_RXD_N")
					(number "32")
				)
				(pin passive line
					(at 35.56 -78.74 180)
					(length 2.54)
					(name "LED3")
					(number "33")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 2.54)
					(name "TEST")
					(number "34")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{RESET}")
					(number "35")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDVARIO")
					(number "36")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(name "USBRBIAS")
					(number "37")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDD33A")
					(number "38")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDVARIO")
					(number "39")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "XI")
					(number "40")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "XO")
					(number "41")
				)
				(pin passive line
					(at 35.56 0 180)
					(length 2.54)
					(hide yes)
					(name "VDD12CORE")
					(number "42")
				)
				(pin passive line
					(at 35.56 -76.2 180)
					(length 2.54)
					(name "PME_MODE")
					(number "43")
				)
				(pin passive line
					(at 35.56 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VDD12A")
					(number "44")
				)
				(pin passive line
					(at 35.56 -17.78 180)
					(length 2.54)
					(name "VDD25_REG_OUT")
					(number "45")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDD33_REG_IN")
					(number "46")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 2.54)
					(name "REF_REXT")
					(number "47")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 2.54)
					(name "REF_FILT")
					(number "48")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 2.54)
					(name "VSS")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
