(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Harwin_M80_2x3_M80-5300642"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 22.86 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Harwin_M80_2x3_M80-5300642"
				(at 22.86 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Harwin_M80_2x3_M80-5300642"
				(at 22.86 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.harwin.com/pdfs/M80-530.pdf"
				(at 22.86 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Datamate J-Tek DIL Male Horizontal 3mm Throughboard Connector, selective gold + tin, with jackscrews, 3+3 contacts"
				(at 22.86 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Harwin"
				(at 22.86 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "M80-5300642"
				(at 22.86 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 22.86 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 22.86 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, HEADER, THT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Harwin_M80_2x3_M80-5300642_0_1")
			(symbol "Harwin_M80_2x3_M80-5300642_1_1"
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "")
					(number "3")
				)
				(pin passive line
					(at 12.7 0 180)
					(length 3.81)
					(name "")
					(number "4")
				)
				(pin passive line
					(at 12.7 -2.54 180)
					(length 3.81)
					(name "")
					(number "5")
				)
				(pin passive line
					(at 12.7 -5.08 180)
					(length 3.81)
					(name "")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
)
