(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MAX3421EETJ+"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 40.64 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MAX3421EETJ+"
				(at 40.64 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MAX3421EETJ+"
				(at 40.64 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max3421e.pdf"
				(at 40.64 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface, ESD-Protected USB Peripheral/Host Controller, USB 2.0, 3 V, 3.6 V, TQFN, 32 Pins"
				(at 40.64 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MAX3421EETJ+"
				(at 40.64 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Maxim Integrated Products"
				(at 40.64 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 40.64 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 40.64 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, TRANSCEIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MAX3421EETJ+_1_1"
				(pin input line
					(at 27.94 -38.1 180)
					(length 2.54)
					(name "GPIN7")
					(number "1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VL")
					(number "2")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin output line
					(at 27.94 0 180)
					(length 2.54)
					(name "GPOUT0")
					(number "4")
				)
				(pin output line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "GPOUT1")
					(number "5")
				)
				(pin output line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "GPOUT2")
					(number "6")
				)
				(pin output line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "GPOUT3")
					(number "7")
				)
				(pin output line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "GPOUT4")
					(number "8")
				)
				(pin output line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "GPOUT5")
					(number "9")
				)
				(pin output line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "GPOUT6")
					(number "10")
				)
				(pin output line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "GPOUT7")
					(number "11")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "~{RES}")
					(number "12")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SCLK")
					(number "13")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "~{SS}")
					(number "14")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "MISO")
					(number "15")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "MOSI")
					(number "16")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 2.54)
					(name "GPX")
					(number "17")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "INT")
					(number "18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "GND")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D-")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D+")
					(number "21")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "VBCOMP")
					(number "22")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "23")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "XI")
					(number "24")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 2.54)
					(name "XO")
					(number "25")
				)
				(pin input line
					(at 27.94 -20.32 180)
					(length 2.54)
					(name "GPIN0")
					(number "26")
				)
				(pin input line
					(at 27.94 -22.86 180)
					(length 2.54)
					(name "GPIN1")
					(number "27")
				)
				(pin input line
					(at 27.94 -25.4 180)
					(length 2.54)
					(name "GPIN2")
					(number "28")
				)
				(pin input line
					(at 27.94 -27.94 180)
					(length 2.54)
					(name "GPIN3")
					(number "29")
				)
				(pin input line
					(at 27.94 -30.48 180)
					(length 2.54)
					(name "GPIN4")
					(number "30")
				)
				(pin input line
					(at 27.94 -33.02 180)
					(length 2.54)
					(name "GPIN5")
					(number "31")
				)
				(pin input line
					(at 27.94 -35.56 180)
					(length 2.54)
					(name "GPIN6")
					(number "32")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "EP")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
