(footprint "Bus_M.2_Socket_Key_M_Amphenol_MDT580M01001"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -5.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Bus_M.2_Socket_Key_M_Amphenol_MDT580M01001"
		(at 0 5.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "Author: Antmicro"
		(at -13 8.499 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -13 9.698 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -13 10.899 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -10 1.425)
		(size 1.1 1.1)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 9.999 1.425)
		(size 1.6 1.6)
		(drill 1.6)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" smd rect
		(at -9.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -9 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -8.75 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -8.5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -8.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -8 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -7.75 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -7.5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -7.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -7 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -6.75 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -6.5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -6.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -6 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -5.75 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -5.5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -5.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -4.75 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -4.5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at -4.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at -4 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at -3.75 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at -3.5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -3.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -3 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -2.75 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -2.5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -2.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -2 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -1.75 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -1.5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at -1.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at -1 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at -0.75 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at -0.5 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at -0.25 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 0 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 0.246 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 0.496 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 0.747 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 0.996 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at 1.249 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at 1.499 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at 1.749 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at 1.999 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at 2.249 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at 2.499 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 2.749 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd rect
		(at 2.999 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd rect
		(at 3.249 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd rect
		(at 3.499 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd rect
		(at 3.749 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd rect
		(at 3.999 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd rect
		(at 4.248 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd rect
		(at 4.498 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 4.748 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "58" smd rect
		(at 4.998 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "67" smd rect
		(at 7.249 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "68" smd rect
		(at 7.498 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "69" smd rect
		(at 7.748 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "70" smd rect
		(at 7.998 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "71" smd rect
		(at 8.249 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "72" smd rect
		(at 8.499 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "73" smd rect
		(at 8.749 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "74" smd rect
		(at 8.999 3.7)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "75" smd rect
		(at 9.249 -3.848)
		(size 0.3 1.55)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP1" smd rect
		(at -10.35 -3.073)
		(size 1.2 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "MP2" smd rect
		(at 10.348 -3.073)
		(size 1.2 2.75)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_mdt580m01001.glb"
		(offset
			(xyz -10.9995 0.1005 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 90)
		)
	)
	(model "antmicro_mdt580m01001.glb"
		(offset
			(xyz 11 -79.5 4.2)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 -90)
		)
	)
)
