(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "MK20DX256VLH7"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 72.39 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "MK20DX256VLH7"
				(at 72.39 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "MK20DX256VLH7"
				(at 72.39 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/part/MK20DX256VLH7"
				(at 72.39 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, K2 USB Series, Kinetis K Family K2x Series Microcontrollers, ARM Cortex-M4, 32 bit, 72 MHz"
				(at 72.39 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "NXP"
				(at 72.39 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MK20DX256VLH7"
				(at 72.39 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 72.39 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 72.39 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MICROCONTROLLER, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "MK20DX256VLH7_1_1"
				(pin bidirectional line
					(at 38.1 -106.68 180)
					(length 2.54)
					(name "PTE0")
					(number "1")
					(alternate "CLKOUT32K" passive line)
				)
				(pin bidirectional line
					(at 38.1 -109.22 180)
					(length 2.54)
					(name "PTE1")
					(number "2")
					(alternate "LLWU_P0" passive line)
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "3")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "USB0_DP")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "USB0_DN")
					(number "6")
				)
				(pin power_out line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VOUT33")
					(number "7")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VREGIN")
					(number "8")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "ADC0_DP0")
					(number "9")
					(alternate "ADC1_DP3" passive line)
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "ADC0_DM0")
					(number "10")
					(alternate "ADC1_DM3" passive line)
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "ADC1_DP0")
					(number "11")
					(alternate "ADC0_DP3" passive line)
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "ADC1_DM0")
					(number "12")
					(alternate "ADC0_DM3" passive line)
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDA")
					(number "13")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "VREFH")
					(number "14")
				)
				(pin power_in line
					(at 0 -99.06 0)
					(length 2.54)
					(name "VREFL")
					(number "15")
				)
				(pin power_in line
					(at 0 -104.14 0)
					(length 2.54)
					(name "VSSA")
					(number "16")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "VREF_OUT")
					(number "17")
					(alternate "ADC1_SE18" passive line)
					(alternate "CMP0_IN5" passive line)
					(alternate "CMP1_IN5" passive line)
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "DAC0_OUT")
					(number "18")
					(alternate "ADC0_SE23" passive line)
					(alternate "CMP1_IN3" passive line)
				)
				(pin output line
					(at 0 -73.66 0)
					(length 2.54)
					(name "XTAL32")
					(number "19")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 2.54)
					(name "EXTAL32")
					(number "20")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VBAT")
					(number "21")
				)
				(pin bidirectional line
					(at 38.1 0 180)
					(length 2.54)
					(name "PTA0")
					(number "22")
				)
				(pin bidirectional line
					(at 38.1 -2.54 180)
					(length 2.54)
					(name "PTA1")
					(number "23")
				)
				(pin bidirectional line
					(at 38.1 -5.08 180)
					(length 2.54)
					(name "PTA2")
					(number "24")
				)
				(pin bidirectional line
					(at 38.1 -7.62 180)
					(length 2.54)
					(name "PTA3")
					(number "25")
				)
				(pin bidirectional line
					(at 38.1 -10.16 180)
					(length 2.54)
					(name "PTA4")
					(number "26")
					(alternate "LLWU_P3" passive line)
				)
				(pin bidirectional line
					(at 38.1 -12.7 180)
					(length 2.54)
					(name "PTA5")
					(number "27")
				)
				(pin bidirectional line
					(at 38.1 -15.24 180)
					(length 2.54)
					(name "PTA12")
					(number "28")
				)
				(pin bidirectional line
					(at 38.1 -17.78 180)
					(length 2.54)
					(name "PTA13")
					(number "29")
					(alternate "LLWU_P4" passive line)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "30")
				)
				(pin power_in line
					(at 0 -109.22 0)
					(length 2.54)
					(name "VSS")
					(number "31")
				)
				(pin bidirectional line
					(at 38.1 -20.32 180)
					(length 2.54)
					(name "PTA18")
					(number "32")
				)
				(pin bidirectional line
					(at 38.1 -22.86 180)
					(length 2.54)
					(name "PTA19")
					(number "33")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 2.54)
					(name "~{RESET_B}")
					(number "34")
				)
				(pin bidirectional line
					(at 38.1 -27.94 180)
					(length 2.54)
					(name "PTB0")
					(number "35")
					(alternate "LLWU_P5" passive line)
				)
				(pin bidirectional line
					(at 38.1 -30.48 180)
					(length 2.54)
					(name "PTB1")
					(number "36")
				)
				(pin bidirectional line
					(at 38.1 -33.02 180)
					(length 2.54)
					(name "PTB2")
					(number "37")
				)
				(pin bidirectional line
					(at 38.1 -35.56 180)
					(length 2.54)
					(name "PTB3")
					(number "38")
				)
				(pin bidirectional line
					(at 38.1 -38.1 180)
					(length 2.54)
					(name "PTB16")
					(number "39")
				)
				(pin bidirectional line
					(at 38.1 -40.64 180)
					(length 2.54)
					(name "PTB17")
					(number "40")
				)
				(pin bidirectional line
					(at 38.1 -43.18 180)
					(length 2.54)
					(name "PTB18")
					(number "41")
				)
				(pin bidirectional line
					(at 38.1 -45.72 180)
					(length 2.54)
					(name "PTB19")
					(number "42")
				)
				(pin bidirectional line
					(at 38.1 -50.8 180)
					(length 2.54)
					(name "PTC0")
					(number "43")
				)
				(pin bidirectional line
					(at 38.1 -53.34 180)
					(length 2.54)
					(name "PTC1")
					(number "44")
					(alternate "LLWU_P6" passive line)
				)
				(pin bidirectional line
					(at 38.1 -55.88 180)
					(length 2.54)
					(name "PTC2")
					(number "45")
				)
				(pin bidirectional line
					(at 38.1 -58.42 180)
					(length 2.54)
					(name "PTC3")
					(number "46")
					(alternate "LLWU_P7" passive line)
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "47")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "48")
				)
				(pin bidirectional line
					(at 38.1 -60.96 180)
					(length 2.54)
					(name "PTC4")
					(number "49")
					(alternate "LLWU_P8" passive line)
				)
				(pin bidirectional line
					(at 38.1 -63.5 180)
					(length 2.54)
					(name "PTC5")
					(number "50")
					(alternate "LLWU_P9" passive line)
				)
				(pin bidirectional line
					(at 38.1 -66.04 180)
					(length 2.54)
					(name "PTC6")
					(number "51")
					(alternate "LLWU_P10" passive line)
				)
				(pin bidirectional line
					(at 38.1 -68.58 180)
					(length 2.54)
					(name "PTC7")
					(number "52")
				)
				(pin bidirectional line
					(at 38.1 -71.12 180)
					(length 2.54)
					(name "PTC8")
					(number "53")
				)
				(pin bidirectional line
					(at 38.1 -73.66 180)
					(length 2.54)
					(name "PTC9")
					(number "54")
				)
				(pin bidirectional line
					(at 38.1 -76.2 180)
					(length 2.54)
					(name "PTC10")
					(number "55")
				)
				(pin bidirectional line
					(at 38.1 -78.74 180)
					(length 2.54)
					(name "PTC11")
					(number "56")
					(alternate "LLWU_P11" passive line)
				)
				(pin bidirectional line
					(at 38.1 -83.82 180)
					(length 2.54)
					(name "PTD0")
					(number "57")
					(alternate "LLWU_P12" passive line)
				)
				(pin bidirectional line
					(at 38.1 -86.36 180)
					(length 2.54)
					(name "PTD1")
					(number "58")
				)
				(pin bidirectional line
					(at 38.1 -88.9 180)
					(length 2.54)
					(name "PTD2")
					(number "59")
					(alternate "LLWU_P13" passive line)
				)
				(pin bidirectional line
					(at 38.1 -91.44 180)
					(length 2.54)
					(name "PTD3")
					(number "60")
				)
				(pin bidirectional line
					(at 38.1 -93.98 180)
					(length 2.54)
					(name "PTD4")
					(number "61")
					(alternate "LLWU_P14" passive line)
				)
				(pin bidirectional line
					(at 38.1 -96.52 180)
					(length 2.54)
					(name "PTD5")
					(number "62")
				)
				(pin bidirectional line
					(at 38.1 -99.06 180)
					(length 2.54)
					(name "PTD6")
					(number "63")
					(alternate "LLWU_P15" passive line)
				)
				(pin bidirectional line
					(at 38.1 -101.6 180)
					(length 2.54)
					(name "PTD7")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
)
