(footprint "Conn_STM_MSAK24025P30"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -10.7 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_STM_MSAK24025P30"
		(at -6.8 0.443 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -11.626 6.174 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -11.626 7.374 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -11.626 8.574 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -7.25 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.75 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.25 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -5.75 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5.25 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -4.75 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -4.25 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.75 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.25 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -2.75 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -2.25 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -1.75 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -1.25 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -0.75 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.25 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 0.249 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 0.749 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 1.249 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 1.749 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 2.249 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 2.749 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 3.249 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 3.749 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 4.249 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 4.749 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 5.249 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 5.749 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 6.249 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 6.749 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 7.249 -1.875)
		(size 0.3 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at -9.18 -0.016)
		(size 2.7 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "SH" smd rect
		(at 9.179 -0.016)
		(size 2.7 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_msak24025p30.glb"
		(offset
			(xyz 0 -0.525 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 180)
		)
	)
)
