(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Conn_STM_MSAK24025P30"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 20.32 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Conn_STM_MSAK24025P30"
				(at 20.32 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Conn_STM_MSAK24025P30"
				(at 20.32 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.stm.com.tw/EEPPulish/files/PE/PE-MSAK24025P30~MSAK24025P50_R.pdf"
				(at 20.32 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Wire to Board Connector pitch 0.5mm"
				(at 20.32 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "MSAK24025P30"
				(at 20.32 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 20.32 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 20.32 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 20.32 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, HEADER, COAXIAL, WIRE-BOARD"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Conn_STM_MSAK24025P30_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "2")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "3")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "4")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "5")
					(number "5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "6")
					(number "6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "7")
					(number "7")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "8")
					(number "8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "9")
					(number "9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "10")
					(number "10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "11")
					(number "11")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "12")
					(number "12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "13")
					(number "13")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "14")
					(number "14")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "15")
					(number "15")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "16")
					(number "16")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "17")
					(number "17")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "18")
					(number "18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "19")
					(number "19")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "20")
					(number "20")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "21")
					(number "21")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "22")
					(number "22")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "23")
					(number "23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "24")
					(number "24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "25")
					(number "25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "26")
					(number "26")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "27")
					(number "27")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 2.54)
					(name "28")
					(number "28")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(name "29")
					(number "29")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 2.54)
					(name "30")
					(number "30")
				)
			)
			(embedded_fonts no)
		)
)
