(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PCM2912A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PCM2912A"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PCM2912A"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcm2912a.pdf?ts=1702485653045&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FPCM2912A"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Audio Codec With USB Interface, TQFP-32"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PCM2912APJTR"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CONTROLLER, IC, USB"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PCM2912A_1_0"
				(pin no_connect line
					(at 27.94 -36.83 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
			)
			(symbol "PCM2912A_1_1"
				(pin power_in line
					(at 0 -50.8 0)
					(length 2.54)
					(name "BGND")
					(number "1")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VBUS")
					(number "2")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "D-")
					(number "3")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "D+")
					(number "4")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "VDD")
					(number "5")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "DGND")
					(number "6")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "XTO")
					(number "7")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "XTI")
					(number "8")
				)
				(pin passive line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "FL")
					(number "9")
				)
				(pin passive line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "FR")
					(number "10")
				)
				(pin passive line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "VCOM1")
					(number "11")
				)
				(pin passive line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "VCOM2")
					(number "12")
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 2.54)
					(name "AGND")
					(number "13")
				)
				(pin passive line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "VCCA")
					(number "15")
				)
				(pin passive line
					(at 30.48 -20.32 180)
					(length 2.54)
					(name "VIN")
					(number "16")
				)
				(pin passive line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "MBIAS")
					(number "17")
				)
				(pin passive line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "VOUTL")
					(number "18")
				)
				(pin passive line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "VCCL")
					(number "19")
				)
				(pin power_in line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "HGND")
					(number "20")
				)
				(pin passive line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "VCCR")
					(number "21")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 2.54)
					(name "VOUTR")
					(number "22")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "MAMP")
					(number "23")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "POWER")
					(number "24")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 2.54)
					(name "PGND")
					(number "25")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCCP")
					(number "26")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "TEST1")
					(number "27")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "TEST0")
					(number "28")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "~{SSPND}")
					(number "29")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "MMUTE")
					(number "30")
				)
				(pin passive line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "~{REC}")
					(number "31")
				)
				(pin passive line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "~{PLAY}")
					(number "32")
				)
			)
			(embedded_fonts no)
		)
)
