(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "PI3USB102GZLEX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "PI3USB102GZLEX"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "PI3USB102GZLEX"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.diodes.com/assets/Datasheets/PI3USB102G.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Switch IC 1 Channel 10-TQFN (1.3x1.6)"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "PI3USB102GZLEX"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Diodes Incorporated"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "PI3USB102GZLEX_0_1")
			(symbol "PI3USB102GZLEX_1_1"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "D+")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D-")
					(number "2")
				)
				(pin power_in line
					(at 20.32 -15.24 180)
					(length 2.54)
					(name "GND")
					(number "3")
				)
				(pin bidirectional line
					(at 20.32 -3.81 180)
					(length 2.54)
					(name "D1-")
					(number "4")
				)
				(pin bidirectional line
					(at 20.32 -1.27 180)
					(length 2.54)
					(name "D1+")
					(number "5")
				)
				(pin bidirectional line
					(at 20.32 -11.43 180)
					(length 2.54)
					(name "D2-")
					(number "6")
				)
				(pin bidirectional line
					(at 20.32 -8.89 180)
					(length 2.54)
					(name "D2+")
					(number "7")
				)
				(pin input line
					(at 0 -11.43 0)
					(length 2.54)
					(name "~{OE}")
					(number "8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{DD}")
					(number "9")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "SEL")
					(number "10")
				)
			)
			(embedded_fonts no)
		)
)
