(footprint "BarrelJack_Pin2mm_PJ-051A"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 1.325 -0.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "BarrelJack_Pin2mm_PJ-051A"
		(at 5.262 10.782 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_line
		(start 5.4 2.4)
		(end 7.2 2.4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 5.4 4.2)
		(end 5.4 2.4)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 7.2 2.4)
		(end 7.2 4.2)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 7.2 4.2)
		(end 5.4 4.2)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at -1.85 12.782 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.85 13.982 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.85 15.182 0)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at 6.3 3.3)
		(size 1.3 1.3)
		(drill 1.3)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole oval
		(at 0 0)
		(size 2.616 1.308)
		(drill oval 2 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 8.6)
		(size 2.616 1.308)
		(drill oval 2 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 0 3.4)
		(size 2.616 1.308)
		(drill oval 2 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 7.3 -0.4)
		(size 2.8 1.3)
		(drill oval 2.3 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole oval
		(at 7.3 9.5)
		(size 2.8 1.3)
		(drill oval 2.3 0.8)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_pj_051a.glb"
		(offset
			(xyz 10.3 -4.55 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 -90)
		)
	)
)
