(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB-A_Switchcraft_RAHUA30E"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB-A_Switchcraft_RAHUA30E"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB-A_Switchcraft_RAHUA30E"
				(at 33.02 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.switchcraft.com/assets/1/6/RAHUA30E_CD.pdf"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB-A (USB TYPE-A) USB 3.2 Gen 1 (USB 3.1 Gen 1, Superspeed (USB 3.0)) Receptacle Connector 9 Position Surface Mount, Right Angle"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RAHUA30E"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Switchcraft"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "USB, CONNECTOR, SMT, HORIZONTAL"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB-A_Switchcraft_RAHUA30E_1_1"
				(pin passive line
					(at 0 0 180)
					(length 2.54)
					(name "VBUS")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -6.35 180)
					(length 2.54)
					(name "D-")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -3.81 180)
					(length 2.54)
					(name "D+")
					(number "3")
				)
				(pin power_in line
					(at 0 -19.05 180)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -11.43 180)
					(length 2.54)
					(name "SSRX-")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -8.89 180)
					(length 2.54)
					(name "SSRX+")
					(number "6")
				)
				(pin power_in line
					(at 0 -21.59 180)
					(length 2.54)
					(name "GND_DRAIN")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -16.51 180)
					(length 2.54)
					(name "SSTX-")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -13.97 180)
					(length 2.54)
					(name "SSTX+")
					(number "9")
				)
				(pin passive line
					(at 0 -24.13 180)
					(length 2.54)
					(name "SHIELD")
					(number "SH")
				)
			)
			(embedded_fonts no)
		)
)
