(footprint "RJ45_RJE361882415"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1.945 22.4 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "RJ45_RJE361882415"
		(at 3.555 23.9 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -16.27 27.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -16.27 28.6 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -16.27 29.8 0)
		(layer "F.Fab")
	)
	(pad "1" thru_hole circle
		(at 0 0 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at -1.27 2.54 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at -2.54 0 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -3.81 2.54 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole circle
		(at -5.08 0 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole circle
		(at -6.35 2.54 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "7" thru_hole circle
		(at -7.62 0 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "8" thru_hole circle
		(at -8.89 2.54 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D1" thru_hole circle
		(at -11.645 -2.71 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D2" thru_hole circle
		(at -9.11 -2.71 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D3" thru_hole circle
		(at 0.22 -2.71 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "D4" thru_hole circle
		(at 2.755 -2.71 90)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at -13.77 2.49 90)
		(size 3 3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at -13.77 15.09 90)
		(size 3 3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at -11.015 7.71 90)
		(size 3 3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at -11.015 13.39 90)
		(size 3 3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 2.125 7.71 90)
		(size 3 3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 2.125 13.39 90)
		(size 3 3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 4.88 2.49 90)
		(size 3 3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "MP" thru_hole circle
		(at 4.88 15.09 90)
		(size 3 3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U1" thru_hole circle
		(at -7.945 11.4)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U2" thru_hole circle
		(at -5.445 11.4)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U3" thru_hole circle
		(at -3.445 11.4)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U4" thru_hole circle
		(at -0.945 11.4)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U5" thru_hole circle
		(at -8.445 9.9)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U6" thru_hole circle
		(at -6.445 9.9)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U7" thru_hole circle
		(at -4.445 9.9)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U8" thru_hole circle
		(at -2.445 9.9)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U9" thru_hole circle
		(at -0.445 9.9)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U10" thru_hole circle
		(at -7.945 8.2)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U11" thru_hole circle
		(at -5.445 8.2)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U12" thru_hole circle
		(at -3.445 8.2)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U13" thru_hole circle
		(at -0.945 8.2)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U14" thru_hole circle
		(at -8.445 6.7)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U15" thru_hole circle
		(at -6.445 6.7)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U16" thru_hole circle
		(at -4.445 6.7)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U17" thru_hole circle
		(at -2.445 6.7)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "U18" thru_hole circle
		(at -0.445 6.7)
		(size 1.35 1.35)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_rje361882415.glb"
		(offset
			(xyz -4.445 3.8 15.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 -180 180)
		)
	)
)
