(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Amphenol_RJE361882415"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 39.37 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Amphenol_RJE361882415"
				(at 39.37 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Amphenol_RJE361882415"
				(at 39.37 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/drawing/p-rje36-188-2xx5.pdf"
				(at 39.37 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Modular Connectors / Ethernet Connectors MODULAR JACK"
				(at 39.37 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RJE361882415"
				(at 39.37 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 39.37 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 39.37 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.37 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "THT, CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Amphenol_RJE361882415_1_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "1")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "2")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "3")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "4")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "5")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "6")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "7")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "8")
					(number "8")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 3.81)
					(name "LED_D1")
					(number "D1")
				)
				(pin passive line
					(at 25.4 -2.54 180)
					(length 3.81)
					(name "LED_D2")
					(number "D2")
				)
				(pin passive line
					(at 25.4 -20.32 180)
					(length 3.81)
					(name "LED_D3")
					(number "D3")
				)
				(pin passive line
					(at 25.4 -22.86 180)
					(length 3.81)
					(name "LED_D4")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "MP")
					(number "MP")
				)
			)
			(symbol "Amphenol_RJE361882415_2_1"
				(text "PORT 1"
					(at 12.7 0 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VBUS")
					(number "U1")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 3.81)
					(name "D-")
					(number "U2")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 3.81)
					(name "D+")
					(number "U3")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 3.81)
					(name "GND")
					(number "U4")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 3.81)
					(name "SSTX+")
					(number "U5")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 3.81)
					(name "SSTX-")
					(number "U6")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 3.81)
					(name "GND_DRAIN")
					(number "U7")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 3.81)
					(name "SSRX+")
					(number "U8")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 3.81)
					(name "SSRX-")
					(number "U9")
				)
			)
			(symbol "Amphenol_RJE361882415_3_1"
				(text "PORT 2"
					(at 12.7 0 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(name "VBUS")
					(number "U10")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 3.81)
					(name "D-")
					(number "U11")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 3.81)
					(name "D+")
					(number "U12")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 3.81)
					(name "GND")
					(number "U13")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 3.81)
					(name "SSTX+")
					(number "U14")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 3.81)
					(name "SSTX-")
					(number "U15")
				)
				(pin power_in line
					(at 0 -21.59 0)
					(length 3.81)
					(name "GND_DRAIN")
					(number "U16")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 3.81)
					(name "SSRX+")
					(number "U17")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 3.81)
					(name "SSRX-")
					(number "U18")
				)
			)
			(embedded_fonts no)
		)
)
