(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RT1710SGQW"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 34.29 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RT1710SGQW"
				(at 34.29 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RT1710SGQW"
				(at 34.29 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.richtek.com/assets/product_file/RT1710/DS1710-00.pdf"
				(at 34.29 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Type C Interface 8-WDFN (2x2)"
				(at 34.29 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "RT1710SGQW"
				(at 34.29 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Richtek"
				(at 34.29 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 34.29 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 34.29 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, USB, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RT1710SGQW_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VCON2")
					(number "1")
				)
				(pin input line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "GND")
					(number "2")
				)
				(pin input line
					(at 20.32 0 180)
					(length 2.54)
					(name "SCL")
					(number "3")
				)
				(pin input line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "SDA")
					(number "4")
				)
				(pin no_connect line
					(at 0 -10.16 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 0 -8.89 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "CCIN")
					(number "7")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "VCON1")
					(number "8")
				)
				(pin input line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "GND_P")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
