(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "RJ45_Bel_SI-51005-F"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 27.94 2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "RJ45_Bel_SI-51005-F"
				(at 27.94 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "RJ45_Bel_SI-51005-F"
				(at 27.94 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://belfuse.com/resources/drawings/magneticsolutions/dr-mag-si-51005-fb.pdf"
				(at 27.94 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Modular connector with magnetics"
				(at 27.94 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Bel Fuse"
				(at 27.94 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SI-51005-F"
				(at 27.94 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 27.94 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 27.94 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "RJ45_Bel_SI-51005-F_0_1")
			(symbol "RJ45_Bel_SI-51005-F_1_1"
				(text "G"
					(at 11.43 -2.54 0)
				)
				(text "G"
					(at 11.43 -25.4 0)
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "D0+")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "D0-")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D1+")
					(number "4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D1-")
					(number "5")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "CTREF")
					(number "6")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "D2+")
					(number "7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "D2-")
					(number "8")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "D3+")
					(number "9")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "D3-")
					(number "10")
				)
				(pin passive line
					(at 19.05 0 180)
					(length 2.54)
					(name "11")
					(number "11")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "12")
					(number "12")
				)
				(pin passive line
					(at 19.05 -25.4 180)
					(length 2.54)
					(name "13")
					(number "13")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "14")
					(number "14")
				)
				(pin passive line
					(at 19.05 -27.94 180)
					(length 2.54)
					(name "SHIELD")
					(number "S")
				)
			)
			(embedded_fonts no)
		)
)
