(footprint "Conn_JST_SUR_1x12_SM12B-SURS-TF-LF-SN"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -1.125 -1.925 0)
		(layer "F.SilkS")
	)
	(property "Value" "JST_SM12B-SURS-TF_LF__SN_"
		(at 9.075 3.045 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -6.55 5.045 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -6.55 6.245 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -6.55 7.445 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.4 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.6 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.8 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.2 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -0.4 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 0.4 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.2 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 2 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 2.8 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 3.6 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 4.4 -1.05)
		(size 0.5 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at -5.7 0.9)
		(size 1.2 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "MP" smd roundrect
		(at 5.7 0.9)
		(size 1.2 1.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "antmicro_sm12b_surs_tf.glb"
		(offset
			(xyz 4.2 6.25 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
