(footprint "D_0201_0603Metric_SP00R6"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(tags "Footprint based on: https://www.littelfuse.com/assetdocs/littelfuse-tvs-diode-array-sp00r6-datasheet?assetguid=5FA6369D-0E65-4A4F-8ED7-0E61EB3C9FBF")
	(property "Reference" "D**"
		(at -0.29 -0.78 0)
		(layer "F.SilkS")
	)
	(property "Value" "D_0201_0603Metric_SP00R6"
		(at 0 1.36 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0.005 -0.005 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0.005 -0.005 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -0.895 2.26 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -0.895 3.46 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -0.895 4.66 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.195 -0.005)
		(size 0.195 0.325)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at 0.205 -0.005)
		(size 0.195 0.325)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_sp00r6_01wtg.glb"
		(offset
			(xyz 0.005 0.005 -0.09)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
