(footprint "UDFN-10_1x2.5mm_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Footprint based on https://www.littelfuse.com/assetdocs/littelfuse-tvs-diode-arrays-sp33r6-series-datasheet?assetguid=17fda436-825f-4698-a26d-e7bf3e493099")
	(property "Reference" "D**"
		(at -0.35 -1.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "UDFN-10_1x2.5mm_P0.5mm"
		(at -1.65 2.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 270)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.63 3.7 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.63 4.9 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.63 6.1 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.4 -1 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -0.4 -0.5 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at 0 0 270)
		(size 0.4 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -0.4 0.5 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.4 1 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0.4 1 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.4 0.5 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.4 -0.5 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0.4 -1 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_sp33r6_04utg.glb"
		(offset
			(xyz 0 0.005 0.3)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -180 0 90)
		)
	)
)
