(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Bel-Fuse_SFP+_2x20_SS-79100-010"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 41.91 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Bel-Fuse_SFP+_2x20_SS-79100-010"
				(at 41.91 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Bel-Fuse_SFP+_2x20_SS-79100-010"
				(at 41.91 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.belfuse.com/resources/datasheets/stewartconnector/ds-STW-SFP-cages.pdf"
				(at 41.91 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "40 Position SFP+ Receptacle with Cage, Ganged (2x1) Connector Press-Fit Through Hole, Right Angle"
				(at 41.91 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "SS-79100-010"
				(at 41.91 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Bel Fuse"
				(at 41.91 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 41.91 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 41.91 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "THT, CONNECTOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Bel-Fuse_SFP+_2x20_SS-79100-010_1_1"
				(text "SFP+\n"
					(at 17.78 0 0)
				)
				(pin passive line
					(at 27.94 -38.1 180)
					(length 3.81)
					(name "SH")
					(number "SH")
				)
				(pin passive line
					(at 27.94 -40.64 180)
					(length 3.81)
					(name "V_{EE}(T)")
					(number "T1")
				)
				(pin open_collector line
					(at 0 -20.32 0)
					(length 3.81)
					(name "TX_{FAULT}")
					(number "T2")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "TX_{DISABLE}")
					(number "T3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "SDA")
					(number "T4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "SCL")
					(number "T5")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "MOD_{ABS}")
					(number "T6")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "RS0")
					(number "T7")
				)
				(pin open_collector line
					(at 0 -17.78 0)
					(length 3.81)
					(name "RX_{LOS}")
					(number "T8")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "RS1")
					(number "T9")
				)
				(pin passive line
					(at 27.94 -43.18 180)
					(length 3.81)
					(name "V_{EE}(R)")
					(number "T10")
				)
				(pin passive line
					(at 27.94 -43.18 180)
					(length 3.81)
					(hide yes)
					(name "V_{EE}(R)")
					(number "T11")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 3.81)
					(name "RD-")
					(number "T12")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 3.81)
					(name "RD+")
					(number "T13")
				)
				(pin passive line
					(at 27.94 -43.18 180)
					(length 3.81)
					(hide yes)
					(name "V_{EE}(R)")
					(number "T14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "V_{CC}(R)")
					(number "T15")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "V_{CC}(T)")
					(number "T16")
				)
				(pin passive line
					(at 27.94 -40.64 180)
					(length 3.81)
					(hide yes)
					(name "V_{EE}(T)")
					(number "T17")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "TD+")
					(number "T18")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "TD-")
					(number "T19")
				)
				(pin passive line
					(at 27.94 -40.64 180)
					(length 3.81)
					(hide yes)
					(name "V_{EE}(T)")
					(number "T20")
				)
			)
			(symbol "Bel-Fuse_SFP+_2x20_SS-79100-010_2_1"
				(text "SFP+\n"
					(at 17.78 0 0)
				)
				(pin passive line
					(at 27.94 -43.18 180)
					(length 3.81)
					(name "V_{EE}(T)")
					(number "L1")
				)
				(pin open_collector line
					(at 0 -20.32 0)
					(length 3.81)
					(name "TX_{FAULT}")
					(number "L2")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "TX_{DISABLE}")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "SDA")
					(number "L4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "SCL")
					(number "L5")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(name "MOD_{ABS}")
					(number "L6")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "RS0")
					(number "L7")
				)
				(pin open_collector line
					(at 0 -17.78 0)
					(length 3.81)
					(name "RX_{LOS}")
					(number "L8")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "RS1")
					(number "L9")
				)
				(pin passive line
					(at 27.94 -40.64 180)
					(length 3.81)
					(name "V_{EE}(R)")
					(number "L10")
				)
				(pin passive line
					(at 27.94 -40.64 180)
					(length 3.81)
					(hide yes)
					(name "V_{EE}(R)")
					(number "L11")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 3.81)
					(name "RD-")
					(number "L12")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 3.81)
					(name "RD+")
					(number "L13")
				)
				(pin passive line
					(at 27.94 -40.64 180)
					(length 3.81)
					(hide yes)
					(name "V_{EE}(R)")
					(number "L14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "V_{CC}(R)")
					(number "L15")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "V_{CC}(T)")
					(number "L16")
				)
				(pin passive line
					(at 27.94 -43.18 180)
					(length 3.81)
					(hide yes)
					(name "V_{EE}(T)")
					(number "L17")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 3.81)
					(name "TD+")
					(number "L18")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "TD-")
					(number "L19")
				)
				(pin passive line
					(at 27.94 -43.18 180)
					(length 3.81)
					(hide yes)
					(name "V_{EE}(T)")
					(number "L20")
				)
			)
			(embedded_fonts no)
		)
)
