(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STUSB4500_QFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STUSB4500_QFN"
				(at 45.72 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STUSB4500_QFN"
				(at 45.72 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/389/dm00489312-1799262.pdf"
				(at 45.72 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Controller USB 2.0 I2C Interface 24-QFN (4x4)"
				(at 45.72 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STUSB4500QTR"
				(at 45.72 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 45.72 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STUSB4500_QFN_1_1"
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CC1DB")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "CC1")
					(number "2")
				)
				(pin no_connect line
					(at 27.94 -31.75 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "CC2")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "CC2DB")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RESET")
					(number "6")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "SCL")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "SDA")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DISCH")
					(number "9")
				)
				(pin power_in line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin output line
					(at 30.48 -10.16 180)
					(length 2.54)
					(name "ATTACH")
					(number "11")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "ADDR0")
					(number "12")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "ADDR1")
					(number "13")
				)
				(pin output line
					(at 30.48 -20.32 180)
					(length 2.54)
					(name "POWER_OK3")
					(number "14")
				)
				(pin output line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "GPIO")
					(number "15")
				)
				(pin output line
					(at 30.48 0 180)
					(length 2.54)
					(name "VBUS_EN_SNK")
					(number "16")
				)
				(pin output line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "A_B_SIDE")
					(number "17")
				)
				(pin input line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "VBUS_VS_DISCH")
					(number "18")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 2.54)
					(name "~{ALERT}")
					(number "19")
				)
				(pin output line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "POWER_OK2")
					(number "20")
				)
				(pin output line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "VREG_1V2")
					(number "21")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VSYS")
					(number "22")
				)
				(pin output line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "VREG_2V7")
					(number "23")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "24")
				)
				(pin power_in line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "EP")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
