(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "STUSB4710AQ1TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "STUSB4710AQ1TR"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "STUSB4710AQ1TR"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/389/stusb4710-1852079.pdf"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USBC PD 2.0 source controller I2C Interface 16-QFN(3x3)"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "STUSB4710AQ1TR"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "STMicroelectronics"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT,CONTROLLER,POE,IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "STUSB4710AQ1TR_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "CC1")
					(number "2")
				)
				(pin bidirectional line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "CC2")
					(number "3")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SCL")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SDA")
					(number "5")
				)
				(pin power_in line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin open_collector line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SEL_PDO3")
					(number "7")
				)
				(pin open_collector line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SEL_PDO2")
					(number "8")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "ADDR0")
					(number "9")
				)
				(pin open_collector line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SEL_PDO4")
					(number "10")
				)
				(pin open_collector line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SEL_PDO5")
					(number "11")
				)
				(pin input line
					(at 30.48 0 180)
					(length 2.54)
					(name "VBUS_SENSE")
					(number "12")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "VBUS_DISCH")
					(number "13")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "VBUS_EN_SRC")
					(number "14")
				)
				(pin power_out line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VREG_1V2")
					(number "15")
				)
				(pin power_out line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VREG_2V7")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
