(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Tag-Connect_TC2050-IDC-NL_2x5_P1.27mm"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 39.37 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Tag-Connect_TC2050-IDC-NL_2x5_P1.27mm"
				(at 39.37 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Tag-Connect_TC2050-IDC-NL_2x5_P1.27mm"
				(at 39.37 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.tag-connect.com/wp-content/uploads/bsk-pdf-manager/TC2050-IDC-NL_Datasheet_8.pdf"
				(at 39.37 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Tag Connect 2x5 1.27mm terminal"
				(at 39.37 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TC2050-IDC-NL"
				(at 39.37 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Tag Connect"
				(at 39.37 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 39.37 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.37 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "POGO-PIN, CONNECTOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Tag-Connect_TC2050-IDC-NL_2x5_P1.27mm_1_1"
				(text "Tag-Connect"
					(at 15.875 1.651 0)
				)
				(text "ALT: 3.3V I2C/JTAG/SPI/SWD/FTDI"
					(at 16.002 -11.938 0)
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "1")
					(number "1")
					(alternate "3V3" passive line)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "2")
					(number "2")
					(alternate "ADBUS3" passive line)
					(alternate "I2C_NC" passive line)
					(alternate "JTAG_TMS" passive line)
					(alternate "SPI_CS" passive line)
					(alternate "SWD_NC" passive line)
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "3")
					(number "3")
					(alternate "GND" passive line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "4")
					(number "4")
					(alternate "ADBUS0" passive line)
					(alternate "I2C_SCL" passive line)
					(alternate "JTAG_TCK" passive line)
					(alternate "SPI_SCK" passive line)
					(alternate "SWD_CLK" passive line)
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "5")
					(number "5")
					(alternate "GND" passive line)
				)
				(pin passive line
					(at 31.75 -10.16 180)
					(length 2.54)
					(name "6")
					(number "6")
					(alternate "ADBUS2" passive line)
					(alternate "I2C_SDA" passive line)
					(alternate "JTAG_TDO" passive line)
					(alternate "SPI_MISO" passive line)
					(alternate "SWD_IO" passive line)
				)
				(pin passive line
					(at 31.75 -7.62 180)
					(length 2.54)
					(name "7")
					(number "7")
					(alternate "NC" no_connect line)
				)
				(pin passive line
					(at 31.75 -5.08 180)
					(length 2.54)
					(name "8")
					(number "8")
					(alternate "ADBUS1" passive line)
					(alternate "I2C_SDA" passive line)
					(alternate "JTAG_TDI" passive line)
					(alternate "SPI_MOSI" passive line)
					(alternate "SWD_IO" passive line)
				)
				(pin passive line
					(at 31.75 -2.54 180)
					(length 2.54)
					(name "9")
					(number "9")
					(alternate "GND" passive line)
				)
				(pin passive line
					(at 31.75 0 180)
					(length 2.54)
					(name "10")
					(number "10")
					(alternate "ADBUS5" passive line)
					(alternate "I2C_NC" passive line)
					(alternate "JTAG_~{RESET}" passive line)
					(alternate "SPI_NC" passive line)
					(alternate "SWD_NC" passive line)
				)
			)
			(embedded_fonts no)
		)
)
