(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TMUXHS4212IRKSR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TMUXHS4212IRKSR"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TMUXHS4212IRKSR"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/TMUXHS4212"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Two-Channel Differential 2:1/1:2 USB3.1 Mux/Demux"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TMUXHS4212IRKSR"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TMUXHS4212IRKSR_1_1"
				(pin no_connect line
					(at 2.54 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "~{OE}")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "A0+")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "A0-")
					(number "4")
				)
				(pin power_in line
					(at 20.32 -33.02 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "A1+")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "A1-")
					(number "8")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "SEL")
					(number "9")
				)
				(pin no_connect line
					(at 2.54 -13.97 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "10")
				)
				(pin passive line
					(at 20.32 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "11")
				)
				(pin bidirectional line
					(at 20.32 -27.94 180)
					(length 2.54)
					(name "C1-")
					(number "12")
				)
				(pin bidirectional line
					(at 20.32 -25.4 180)
					(length 2.54)
					(name "C1+")
					(number "13")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "C0-")
					(number "14")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "C0+")
					(number "15")
				)
				(pin bidirectional line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "B1-")
					(number "16")
				)
				(pin bidirectional line
					(at 20.32 -17.78 180)
					(length 2.54)
					(name "B1+")
					(number "17")
				)
				(pin bidirectional line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "B0-")
					(number "18")
				)
				(pin bidirectional line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "B0+")
					(number "19")
				)
				(pin passive line
					(at 20.32 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "20")
				)
				(pin passive line
					(at 20.32 -33.02 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
