(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TMUXHS4412RUAR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TMUXHS4412RUAR"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TMUXHS4412RUAR"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/TMUXHS4412"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Four-Channel Differential 2:1/1:2 PCIe/USB3.1 Mux/Demux"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TMUXHS4412RUAR"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TMUXHS4412RUAR_1_0"
				(pin no_connect line
					(at 2.54 -48.26 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin no_connect line
					(at 2.54 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "5")
				)
				(pin power_in line
					(at 20.32 -68.58 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin passive line
					(at 20.32 -68.58 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "9")
				)
				(pin no_connect line
					(at 2.54 -33.02 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "13")
				)
				(pin passive line
					(at 20.32 -68.58 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "16")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "SEL")
					(number "17")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "PD")
					(number "18")
				)
				(pin no_connect line
					(at 2.54 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "19")
				)
				(pin no_connect line
					(at 2.54 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin passive line
					(at 20.32 -68.58 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
				(pin bidirectional line
					(at 20.32 -58.42 180)
					(length 2.54)
					(name "DB3N")
					(number "22")
				)
				(pin bidirectional line
					(at 20.32 -55.88 180)
					(length 2.54)
					(name "DB3P")
					(number "23")
				)
				(pin bidirectional line
					(at 20.32 -43.18 180)
					(length 2.54)
					(name "DB2N")
					(number "26")
				)
				(pin passive line
					(at 20.32 -68.58 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "30")
				)
				(pin passive line
					(at 20.32 -68.58 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "39")
				)
				(pin no_connect line
					(at 2.54 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "40")
				)
				(pin no_connect line
					(at 2.54 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "41")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 2.54)
					(name "RSVD")
					(number "42")
				)
				(pin passive line
					(at 20.32 -68.58 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "43")
				)
			)
			(symbol "TMUXHS4412RUAR_1_1"
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D0P")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D0N")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "D1P")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "D1N")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "D2P")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "D2N")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 2.54)
					(name "D3P")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "D3N")
					(number "15")
				)
				(pin bidirectional line
					(at 20.32 -52.07 180)
					(length 2.54)
					(name "DA3N")
					(number "24")
				)
				(pin bidirectional line
					(at 20.32 -49.53 180)
					(length 2.54)
					(name "DA3P")
					(number "25")
				)
				(pin bidirectional line
					(at 20.32 -40.64 180)
					(length 2.54)
					(name "DB2P")
					(number "27")
				)
				(pin bidirectional line
					(at 20.32 -36.83 180)
					(length 2.54)
					(name "DA2N")
					(number "28")
				)
				(pin bidirectional line
					(at 20.32 -34.29 180)
					(length 2.54)
					(name "DA2P")
					(number "29")
				)
				(pin bidirectional line
					(at 20.32 -27.94 180)
					(length 2.54)
					(name "DB1N")
					(number "31")
				)
				(pin bidirectional line
					(at 20.32 -25.4 180)
					(length 2.54)
					(name "DB1P")
					(number "32")
				)
				(pin bidirectional line
					(at 20.32 -21.59 180)
					(length 2.54)
					(name "DA1N")
					(number "33")
				)
				(pin bidirectional line
					(at 20.32 -19.05 180)
					(length 2.54)
					(name "DA1P")
					(number "34")
				)
				(pin bidirectional line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "DB0N")
					(number "35")
				)
				(pin bidirectional line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "DB0P")
					(number "36")
				)
				(pin bidirectional line
					(at 20.32 -6.35 180)
					(length 2.54)
					(name "DA0N")
					(number "37")
				)
				(pin bidirectional line
					(at 20.32 -3.81 180)
					(length 2.54)
					(name "DA0P")
					(number "38")
				)
			)
			(embedded_fonts no)
		)
)
