(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS25820DSST"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS25820DSST"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS25820DSST"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps25820.pdf?ts=1624891405505&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTPS25820"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface IC USB Type-C source controller and 1.5A power switch 12-WSON -40°C to 125°C"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS25820DSST"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS25820DSST_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "IN")
					(number "1")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "IN")
					(number "2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CHG")
					(number "3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "EN")
					(number "4")
				)
				(pin output line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "~{FAULT}")
					(number "5")
				)
				(pin output line
					(at 20.32 -16.51 180)
					(length 2.54)
					(name "~{SINK}")
					(number "6")
				)
				(pin output line
					(at 20.32 -20.32 180)
					(length 2.54)
					(name "~{POL}")
					(number "7")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "REF")
					(number "8")
				)
				(pin bidirectional line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "CC1")
					(number "9")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin bidirectional line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "CC2")
					(number "11")
				)
				(pin power_out line
					(at 20.32 0 180)
					(length 2.54)
					(name "OUT")
					(number "12")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
)
