(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS26750SRSMR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS26750SRSMR"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS26750SRSMR"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps26750.pdf"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Type-C® and USB Power Delivery (PD) 3.1 controller with 240-W extended power range support"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS26750SRSMR"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, CONTROLLER, IC, INTERFACE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS26750SRSMR_1_1"
				(pin power_out line
					(at 35.56 -5.08 180)
					(length 2.54)
					(name "LDO_3V3")
					(number "1")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "ADCIN1")
					(number "2")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "ADCIN2")
					(number "3")
				)
				(pin power_out line
					(at 35.56 -7.62 180)
					(length 2.54)
					(name "LDO_1V5")
					(number "4")
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 2.54)
					(name "GPIO0")
					(number "5")
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 2.54)
					(name "GPIO1")
					(number "6")
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 2.54)
					(name "GPIO2")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "I2C_T_SDA")
					(number "8")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "I2C_T_SCL")
					(number "9")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 2.54)
					(name "~{I2C_T_IRQ}")
					(number "10")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 2.54)
					(name "GND")
					(number "11")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "12")
				)
				(pin bidirectional line
					(at 35.56 -45.72 180)
					(length 2.54)
					(name "GPIO11")
					(number "13")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "I2C_C_SDA")
					(number "15")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "I2C_C_SCL")
					(number "16")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 2.54)
					(name "~{I2C_C_IRQ}")
					(number "17")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 2.54)
					(name "GPIO3")
					(number "18")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "19")
				)
				(pin output line
					(at 35.56 -12.7 180)
					(length 2.54)
					(name "POWER_PATH_EN")
					(number "20")
				)
				(pin no_connect line
					(at 2.54 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "21")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 2.54)
					(name "GPIO4/USB_P/LD1")
					(number "22")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 2.54)
					(name "GPIO5/USB_N/LD2")
					(number "23")
				)
				(pin bidirectional line
					(at 35.56 -17.78 180)
					(length 2.54)
					(name "CC1")
					(number "24")
				)
				(pin bidirectional line
					(at 35.56 -20.32 180)
					(length 2.54)
					(name "CC2")
					(number "25")
				)
				(pin power_out line
					(at 35.56 0 180)
					(length 2.54)
					(name "VBUS")
					(number "26")
				)
				(pin passive line
					(at 35.56 0 180)
					(length 2.54)
					(hide yes)
					(name "VBUS")
					(number "27")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "PP5V")
					(number "28")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "PP5V")
					(number "29")
				)
				(pin bidirectional line
					(at 35.56 -43.18 180)
					(length 2.54)
					(name "GPIO7")
					(number "30")
				)
				(pin bidirectional line
					(at 35.56 -40.64 180)
					(length 2.54)
					(name "GPIO6")
					(number "31")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VIN_3V3")
					(number "32")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
