(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS65983BAZBHR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 73.66 2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS65983BAZBHR"
				(at 73.66 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS65983BAZBHR"
				(at 73.66 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps65983b.pdf?ts=1678712702533&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTPS65983B"
				(at 73.66 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface IC Universal USB Type-C and Power Delivery (PD) 3.0 controller 96-NFBGA -10°C to 85"
				(at 73.66 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS65983BAZBHR"
				(at 73.66 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 73.66 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 73.66 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 73.66 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS65983BAZBHR_0_1")
			(symbol "TPS65983BAZBHR_1_1"
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(name "GND")
					(number "A1")
				)
				(pin power_out line
					(at 58.42 -22.86 180)
					(length 3.81)
					(name "LDO_1V8D")
					(number "A2")
				)
				(pin output line
					(at 0 -76.2 0)
					(length 3.81)
					(name "SPI_CLK")
					(number "A3")
				)
				(pin input line
					(at 0 -81.28 0)
					(length 3.81)
					(name "SPI_POCI")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "I2C_SDA2")
					(number "A5")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PP_HV")
					(number "A6")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "PP_HV")
					(number "A7")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "PP_HV")
					(number "A8")
				)
				(pin output line
					(at 58.42 0 180)
					(length 3.81)
					(name "HV_GATE2")
					(number "A9")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "SENSEN")
					(number "A10")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PP_5V0")
					(number "A11")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VDDIO")
					(number "B1")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GPIO0(HD3_AMSEL)")
					(number "B2")
				)
				(pin output line
					(at 0 -83.82 0)
					(length 3.81)
					(name "SPI_CSZ")
					(number "B3")
				)
				(pin output line
					(at 0 -78.74 0)
					(length 3.81)
					(name "SPI_PICO")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "I2C_SCL2")
					(number "B5")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 3.81)
					(name "I2C_IRQ2Z")
					(number "B6")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "PP_HV")
					(number "B7")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B8")
				)
				(pin output line
					(at 58.42 2.54 180)
					(length 3.81)
					(name "HV_GATE1")
					(number "B9")
				)
				(pin input line
					(at 0 2.54 0)
					(length 3.81)
					(name "SENSEP")
					(number "B10")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "PP_5V0")
					(number "B11")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 3.81)
					(name "I2C_IRQ1Z")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "GPIO1(CONFIG0)")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "GPIO4(HPD_TXRX)")
					(number "C10")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "PP_5V0")
					(number "C11")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "I2C_SDA1")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "I2C_SCL1")
					(number "D2")
				)
				(pin bidirectional line
					(at 58.42 -83.82 180)
					(length 3.81)
					(name "DEBUG_CTL2(GPIO17,_I2CADDR_B5)")
					(number "D5")
				)
				(pin input line
					(at 58.42 -106.68 180)
					(length 3.81)
					(name "HRESET")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "GPIO7")
					(number "D7")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D8")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "GPIO2")
					(number "D10")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "PP_5V0")
					(number "D11")
				)
				(pin power_out line
					(at 58.42 -27.94 180)
					(length 3.81)
					(name "LDO_BMC")
					(number "E1")
				)
				(pin output line
					(at 0 -99.06 0)
					(length 3.81)
					(name "UART_TX")
					(number "E2")
				)
				(pin bidirectional line
					(at 58.42 -86.36 180)
					(length 3.81)
					(name "DEBUG_CTL1(GPIO16,_I2CADDR_B4)")
					(number "E4")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E8")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "GPIO5(HPD_RX)")
					(number "E10")
				)
				(pin bidirectional line
					(at 58.42 -101.6 180)
					(length 3.81)
					(name "MRESET(GPIO11)")
					(number "E11")
				)
				(pin bidirectional line
					(at 58.42 -91.44 180)
					(length 3.81)
					(name "I2C_ADDR")
					(number "F1")
				)
				(pin input line
					(at 0 -96.52 0)
					(length 3.81)
					(name "UART_RX")
					(number "F2")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 3.81)
					(name "SWD_DATA")
					(number "F4")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F6")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F7")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin bidirectional line
					(at 58.42 -111.76 180)
					(length 3.81)
					(name "BUSPOWERZ(GPIO10)")
					(number "F10")
				)
				(pin bidirectional line
					(at 58.42 -96.52 180)
					(length 3.81)
					(name "RESETZ(GPIO9)")
					(number "F11")
				)
				(pin power_out line
					(at 58.42 -12.7 180)
					(length 3.81)
					(name "LDO_3V3")
					(number "G1")
				)
				(pin bidirectional line
					(at 58.42 -116.84 180)
					(length 3.81)
					(name "R_OSC")
					(number "G2")
				)
				(pin input line
					(at 0 -91.44 0)
					(length 3.81)
					(name "SWD_CLK")
					(number "G4")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G6")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G7")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G8")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "GPIO6")
					(number "G10")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GPIO3(HD3_EN)")
					(number "G11")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VIN_3V3")
					(number "H1")
				)
				(pin power_out line
					(at 58.42 -7.62 180)
					(length 3.81)
					(name "VOUT_3V3")
					(number "H2")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H4")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "GPIO8")
					(number "H6")
				)
				(pin output line
					(at 58.42 -121.92 180)
					(length 3.81)
					(name "SS")
					(number "H7")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PP_CABLE")
					(number "H10")
				)
				(pin power_in line
					(at 58.42 -5.08 180)
					(length 3.81)
					(name "VBUS")
					(number "H11")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 3.81)
					(name "AUX_P")
					(number "J1")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 3.81)
					(name "AUX_N")
					(number "J2")
				)
				(pin power_in line
					(at 58.42 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "VBUS")
					(number "J10")
				)
				(pin power_in line
					(at 58.42 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "VBUS")
					(number "J11")
				)
				(pin power_out line
					(at 58.42 -17.78 180)
					(length 3.81)
					(name "LDO_1V8A")
					(number "K1")
				)
				(pin bidirectional line
					(at 58.42 -76.2 180)
					(length 3.81)
					(name "DEBUG2(GPIO14,HD3POL)")
					(number "K2")
				)
				(pin bidirectional line
					(at 58.42 -71.12 180)
					(length 3.81)
					(name "DEBUG4(GPIO12,CONFIG2)")
					(number "K3")
				)
				(pin output line
					(at 0 -106.68 0)
					(length 3.81)
					(name "LSX_P2R")
					(number "K4")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 3.81)
					(name "USB_RP_N")
					(number "K5")
				)
				(pin bidirectional line
					(at 58.42 -48.26 180)
					(length 3.81)
					(name "C_USB_TP")
					(number "K6")
				)
				(pin bidirectional line
					(at 58.42 -55.88 180)
					(length 3.81)
					(name "C_USB_BP")
					(number "K7")
				)
				(pin bidirectional line
					(at 58.42 -63.5 180)
					(length 3.81)
					(name "C_SBU1")
					(number "K8")
				)
				(pin bidirectional line
					(at 58.42 -40.64 180)
					(length 3.81)
					(name "RPD_G1")
					(number "K9")
				)
				(pin bidirectional line
					(at 58.42 -43.18 180)
					(length 3.81)
					(name "RPD_G2")
					(number "K10")
				)
				(pin power_in line
					(at 58.42 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "VBUS")
					(number "K11")
				)
				(pin power_in line
					(at 0 -127 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L1")
				)
				(pin bidirectional line
					(at 58.42 -78.74 180)
					(length 3.81)
					(name "DEBUG1(GPIO15)")
					(number "L2")
				)
				(pin bidirectional line
					(at 58.42 -73.66 180)
					(length 3.81)
					(name "DEBUG3(GPIO13,CONFIG1)")
					(number "L3")
				)
				(pin input line
					(at 0 -104.14 0)
					(length 3.81)
					(name "LSX_R2P")
					(number "L4")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 3.81)
					(name "USB_RP_P")
					(number "L5")
				)
				(pin bidirectional line
					(at 58.42 -50.8 180)
					(length 3.81)
					(name "C_USB_TN")
					(number "L6")
				)
				(pin bidirectional line
					(at 58.42 -58.42 180)
					(length 3.81)
					(name "C_USB_BN")
					(number "L7")
				)
				(pin bidirectional line
					(at 58.42 -66.04 180)
					(length 3.81)
					(name "C_SBU2")
					(number "L8")
				)
				(pin bidirectional line
					(at 58.42 -33.02 180)
					(length 3.81)
					(name "C_CC1")
					(number "L9")
				)
				(pin bidirectional line
					(at 58.42 -35.56 180)
					(length 3.81)
					(name "C_CC2")
					(number "L10")
				)
				(pin no_connect line
					(at 3.81 -123.19 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L11")
				)
			)
			(embedded_fonts no)
		)
)
