(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TPS65988DHRSHR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 49.53 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TPS65988DHRSHR"
				(at 49.53 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TPS65988DHRSHR"
				(at 49.53 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps65988.pdf?ts=1662726631004&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTPS65988"
				(at 49.53 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB, Type-C Controller PMIC 56-VQFN (7x7)"
				(at 49.53 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TPS65988DHRSHR "
				(at 49.53 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 49.53 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 49.53 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 49.53 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, CONTROLLER, IC, USB"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TPS65988DHRSHR_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VIN_3V3")
					(number "5")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "ADCIN1")
					(number "6")
				)
				(pin power_out line
					(at 0 -5.08 0)
					(length 2.54)
					(name "LDO_3V3")
					(number "9")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 2.54)
					(name "ADCIN2")
					(number "10")
				)
				(pin bidirectional line
					(at 35.56 0 180)
					(length 2.54)
					(name "GPIO0")
					(number "16")
				)
				(pin bidirectional line
					(at 35.56 -2.54 180)
					(length 2.54)
					(name "GPIO1")
					(number "17")
				)
				(pin bidirectional line
					(at 35.56 -5.08 180)
					(length 2.54)
					(name "GPIO2")
					(number "18")
				)
				(pin power_in line
					(at 0 -64.77 0)
					(length 2.54)
					(name "GND")
					(number "20")
				)
				(pin bidirectional line
					(at 35.56 -13.97 180)
					(length 2.54)
					(name "I2C3_SCL")
					(number "21")
					(alternate "GPIO5" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -16.51 180)
					(length 2.54)
					(name "I2C3_SDA")
					(number "22")
					(alternate "GPIO6" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -19.05 180)
					(length 2.54)
					(name "~{I2C3_IRQ}")
					(number "23")
					(alternate "GPIO7" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -54.61 180)
					(length 2.54)
					(name "I2C1_SCL")
					(number "27")
				)
				(pin bidirectional line
					(at 35.56 -57.15 180)
					(length 2.54)
					(name "I2C1_SDA")
					(number "28")
				)
				(pin output line
					(at 35.56 -52.07 180)
					(length 2.54)
					(name "~{I2C1_IRQ}")
					(number "29")
				)
				(pin bidirectional line
					(at 35.56 -7.62 180)
					(length 2.54)
					(name "HPD1")
					(number "30")
					(alternate "GPIO3" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -10.16 180)
					(length 2.54)
					(name "HPD2")
					(number "31")
					(alternate "GPIO4" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -64.77 180)
					(length 2.54)
					(name "I2C2_SCL")
					(number "32")
				)
				(pin bidirectional line
					(at 35.56 -67.31 180)
					(length 2.54)
					(name "I2C2_SDA")
					(number "33")
				)
				(pin output line
					(at 35.56 -62.23 180)
					(length 2.54)
					(name "~{I2C2_IRQ}")
					(number "34")
				)
				(pin power_out line
					(at 0 -2.54 0)
					(length 2.54)
					(name "LDO_1V8")
					(number "35")
				)
				(pin bidirectional line
					(at 35.56 -22.86 180)
					(length 2.54)
					(name "SPI_POCI")
					(number "36")
					(alternate "GPIO8" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -25.4 180)
					(length 2.54)
					(name "SPI_PICO")
					(number "37")
					(alternate "GPIO9" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -27.94 180)
					(length 2.54)
					(name "SPI_CLK")
					(number "38")
					(alternate "GPIO10" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -30.48 180)
					(length 2.54)
					(name "~{SPI_CS}")
					(number "39")
					(alternate "GPIO11" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -34.29 180)
					(length 2.54)
					(name "GPIO12")
					(number "40")
				)
				(pin bidirectional line
					(at 35.56 -36.83 180)
					(length 2.54)
					(name "GPIO13")
					(number "41")
				)
				(pin bidirectional line
					(at 35.56 -39.37 180)
					(length 2.54)
					(name "PWM1")
					(number "42")
					(alternate "GPIO14" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -41.91 180)
					(length 2.54)
					(name "PWM2")
					(number "43")
					(alternate "GPIO15" bidirectional line)
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "HRESET")
					(number "44")
				)
				(pin bidirectional line
					(at 35.56 -44.45 180)
					(length 2.54)
					(name "PP_EXT1")
					(number "48")
					(alternate "GPIO16" bidirectional line)
				)
				(pin bidirectional line
					(at 35.56 -46.99 180)
					(length 2.54)
					(name "PP_EXT2")
					(number "49")
					(alternate "GPIO17" bidirectional line)
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "51")
				)
				(pin power_in line
					(at 0 -67.31 0)
					(length 2.54)
					(name "GND_EP")
					(number "59")
				)
			)
			(symbol "TPS65988DHRSHR_2_1"
				(pin passive line
					(at 31.75 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "DRAIN1")
					(number "8")
				)
				(pin bidirectional line
					(at 31.75 0 180)
					(length 2.54)
					(name "PP_HV1")
					(number "11")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "VBUS1")
					(number "13")
				)
				(pin passive line
					(at 31.75 -15.24 180)
					(length 2.54)
					(name "DRAIN1")
					(number "15")
				)
				(pin passive line
					(at 31.75 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "DRAIN1")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "C1_CC1")
					(number "24")
				)
				(pin power_in line
					(at 31.75 -3.81 180)
					(length 2.54)
					(name "PP1_CABLE")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "C1_CC2")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "C1_USB_P")
					(number "50")
					(alternate "GPIO18" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "C1_USB_N")
					(number "53")
					(alternate "GPIO19" bidirectional line)
				)
				(pin passive line
					(at 31.75 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "DRAIN1")
					(number "58")
				)
			)
			(symbol "TPS65988DHRSHR_3_1"
				(pin bidirectional line
					(at 31.75 0 180)
					(length 2.54)
					(name "PP_HV2")
					(number "1")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "VBUS2")
					(number "3")
				)
				(pin passive line
					(at 31.75 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "DRAIN2")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "C2_CC1")
					(number "45")
				)
				(pin power_in line
					(at 31.75 -3.81 180)
					(length 2.54)
					(name "PP2_CABLE")
					(number "46")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "C2_CC2")
					(number "47")
				)
				(pin passive line
					(at 31.75 -15.24 180)
					(length 2.54)
					(name "DRAIN2")
					(number "52")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "C2_USB_P")
					(number "54")
					(alternate "GPIO20" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "C2_USB_N")
					(number "55")
					(alternate "GPIO21" bidirectional line)
				)
				(pin passive line
					(at 31.75 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "DRAIN2")
					(number "56")
				)
				(pin passive line
					(at 31.75 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "DRAIN2")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
)
