(footprint "WQFN-40_1EP_6x3mm_Pitch0.4mm_EP4.7x2.7mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "WQFN-40_1EP_6x3mm_Pitch0.4mm_EP4.7x2.7mm"
		(at 0 3.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.101 4.099 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.101 5.099 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.101 6.099 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -2.9 -1.401 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.9 -1 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.9 -0.6 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.9 -0.202 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.9 0.2 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.9 0.598 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.9 0.998 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -2.9 1.398 90)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at -2.202 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at -1.801 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at -1.401 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at -1 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -0.6 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at -0.202 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 0.2 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 0.598 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "17" smd roundrect
		(at 0.998 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "18" smd roundrect
		(at 1.398 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "19" smd roundrect
		(at 1.8 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "20" smd roundrect
		(at 2.2 1.898 180)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "21" smd roundrect
		(at 2.898 1.398 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "22" smd roundrect
		(at 2.898 0.998 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "23" smd roundrect
		(at 2.898 0.598 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "24" smd roundrect
		(at 2.898 0.2 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "25" smd roundrect
		(at 2.898 -0.202 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "26" smd roundrect
		(at 2.898 -0.6 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "27" smd roundrect
		(at 2.898 -1 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "28" smd roundrect
		(at 2.898 -1.401 270)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "29" smd roundrect
		(at 2.2 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "30" smd roundrect
		(at 1.8 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "31" smd roundrect
		(at 1.398 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "32" smd roundrect
		(at 0.998 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "33" smd roundrect
		(at 0.598 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "34" smd roundrect
		(at 0.2 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "35" smd roundrect
		(at -0.202 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "36" smd roundrect
		(at -0.6 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "37" smd roundrect
		(at -1 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "38" smd roundrect
		(at -1.401 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "39" smd roundrect
		(at -1.801 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "40" smd roundrect
		(at -2.202 -1.901)
		(size 0.2 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "41" smd roundrect
		(at -1.5 -0.652 180)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "41" smd roundrect
		(at -1.5 0.748 180)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "41" smd roundrect
		(at 0 0 180)
		(size 4.7 2.7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.01851851852)
	)
	(pad "41" smd roundrect
		(at 0.05 -0.652 180)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "41" smd roundrect
		(at 0.05 0.748 180)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "41" smd roundrect
		(at 1.499 -0.652 180)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "41" smd roundrect
		(at 1.499 0.748 180)
		(size 1 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05)
	)
	(embedded_fonts no)
	(model "antmicro_tusb1046_dcirnqt.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
