(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TUSB1046-DCIRNQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TUSB1046-DCIRNQ"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TUSB1046-DCIRNQ"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/sllsew2d/sllsew2d.pdf?ts=1662107117482&ref_url=https%253A%252F%252Fwww.google.com%252F"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Analog & Digital Crosspoint ICs USB Type-C DP ALT Mode, 10-Gbps linear redriver crosspoint switch 40-WQFN 0°C to 70°C"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TUSB1046-DCIRNQT"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TUSB1046-DCIRNQ_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "1")
				)
				(pin input line
					(at 25.4 -58.42 180)
					(length 2.54)
					(name "DPEQ1")
					(number "2")
				)
				(pin input line
					(at 25.4 -53.34 180)
					(length 2.54)
					(name "SSEQ1")
					(number "3")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "SSRX_N")
					(number "4")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "SSRX_P")
					(number "5")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "6")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "SSTX_N")
					(number "7")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SSTX_P")
					(number "8")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "DP0_P")
					(number "9")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 2.54)
					(name "DP0_N")
					(number "10")
				)
				(pin input line
					(at 25.4 -50.8 180)
					(length 2.54)
					(name "SSEQ0/A0")
					(number "11")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "DP1_P")
					(number "12")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 2.54)
					(name "DP1_N")
					(number "13")
				)
				(pin input line
					(at 25.4 -55.88 180)
					(length 2.54)
					(name "DPEQ0/A1")
					(number "14")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 2.54)
					(name "DP2_P")
					(number "15")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 2.54)
					(name "DP2_N")
					(number "16")
				)
				(pin input line
					(at 25.4 -48.26 180)
					(length 2.54)
					(name "I2C_EN")
					(number "17")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 2.54)
					(name "DP3_P")
					(number "18")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 2.54)
					(name "DP3_N")
					(number "19")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "20")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "FLIP/SCL")
					(number "21")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "CTL0/SDA")
					(number "22")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "CTL1/HPDIN")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "AUX_P")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "AUX_N")
					(number "25")
				)
				(pin bidirectional line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "SBU2")
					(number "26")
				)
				(pin bidirectional line
					(at 25.4 -30.48 180)
					(length 2.54)
					(name "SBU1")
					(number "27")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "CAD_SNK/RSVD1")
					(number "29")
					(alternate "CAD_SNK" bidirectional line)
					(alternate "RSVD1" no_connect line)
				)
				(pin input line
					(at 25.4 0 180)
					(length 2.54)
					(name "RX1_P")
					(number "30")
				)
				(pin input line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "RX1_N")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "HPDIN/RSVD2")
					(number "32")
					(alternate "HPDIN" bidirectional line)
					(alternate "RSVD2" no_connect line)
				)
				(pin output line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "TX1_P")
					(number "33")
				)
				(pin output line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "TX1_N")
					(number "34")
				)
				(pin input line
					(at 25.4 -63.5 180)
					(length 2.54)
					(name "EQ1")
					(number "35")
				)
				(pin output line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "TX2_N")
					(number "36")
				)
				(pin output line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "TX2_P")
					(number "37")
				)
				(pin input line
					(at 25.4 -60.96 180)
					(length 2.54)
					(name "EQ0")
					(number "38")
				)
				(pin input line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "RX2_N")
					(number "39")
				)
				(pin input line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "RX2_P")
					(number "40")
				)
				(pin power_in line
					(at 25.4 -73.66 180)
					(length 2.54)
					(name "GND")
					(number "41")
				)
			)
			(embedded_fonts no)
		)
)
