(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TUSB1106RSVR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 36.83 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TUSB1106RSVR"
				(at 36.83 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TUSB1106RSVR"
				(at 36.83 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tusb1106.pdf?ts=1672125307635&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTUSB1106%252Fpart-details%252FTUSB1106RTZR"
				(at 36.83 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "1/1 Transceiver Half USB 2.0 16-UQFN"
				(at 36.83 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TUSB1106RSVR"
				(at 36.83 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 36.83 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 36.83 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 36.83 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TUSB1106RSVR_1_1"
				(pin input line
					(at 22.86 -5.08 180)
					(length 2.54)
					(name "~{OE}")
					(number "1")
				)
				(pin output line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "RCV")
					(number "2")
				)
				(pin output line
					(at 22.86 -15.24 180)
					(length 2.54)
					(name "VP")
					(number "3")
				)
				(pin output line
					(at 22.86 -12.7 180)
					(length 2.54)
					(name "VM")
					(number "4")
				)
				(pin input line
					(at 22.86 -7.62 180)
					(length 2.54)
					(name "SUSPND")
					(number "5")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin power_in line
					(at 22.86 0 180)
					(length 2.54)
					(name "VCCIO")
					(number "7")
				)
				(pin input line
					(at 22.86 -10.16 180)
					(length 2.54)
					(name "SPEEED")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "D-")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "D+")
					(number "10")
				)
				(pin input line
					(at 22.86 -17.78 180)
					(length 2.54)
					(name "VPO")
					(number "11")
				)
				(pin input line
					(at 22.86 -20.32 180)
					(length 2.54)
					(name "VMO")
					(number "12")
				)
				(pin power_out line
					(at 0 0 0)
					(length 2.54)
					(name "VREG")
					(number "13")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCC")
					(number "14")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VPU")
					(number "15")
				)
				(pin input line
					(at 22.86 -25.4 180)
					(length 2.54)
					(name "SOFTCON")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
