(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TUSB2046BIRHBR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TUSB2046BIRHBR"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TUSB2046BIRHBR"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tusb2046b.pdf?HQS=dis-dk-null-digikeymode-dsf-pf-null-wwe&ts=1755612051596&ref_url=https%253A%252F%252Fwww.ti.com%252Fgeneral%252Fdocs%252Fsuppproductinfo.tsp%253FdistId%253D10%2526gotoUrl%253Dhttps%253A%252F%252Fwww.ti.com%252Flit%252Fgpn%252Ftusb2046b"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "4-Port USB Hub Controller, USB 2.0,  32-VQFN (5x5), Optional Serial EEPROM Interface"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TUSB2046BIRHBR"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TUSB2046BIRHBR_1_1"
				(text "PORT 1"
					(at 25.4 -11.43 0)
				)
				(text "PORT 2"
					(at 25.4 -26.67 0)
				)
				(text "PORT 3"
					(at 25.4 -41.91 0)
				)
				(text "PORT 4"
					(at 25.4 -57.15 0)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "D0_P")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "D0_N")
					(number "2")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "3")
				)
				(pin input line
					(at 0 -8.89 0)
					(length 2.54)
					(name "~{RESET}")
					(number "4")
				)
				(pin output line
					(at 0 -41.91 0)
					(length 2.54)
					(name "EECLK")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "EEDATA")
					(number "6")
					(alternate "GANGED" passive line)
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "BUSPWR")
					(number "8")
				)
				(pin output line
					(at 40.64 -3.81 180)
					(length 2.54)
					(name "~{PWRON1}")
					(number "9")
				)
				(pin input line
					(at 40.64 -1.27 180)
					(length 2.54)
					(name "~{OVRCUR1}")
					(number "10")
				)
				(pin bidirectional line
					(at 40.64 -8.89 180)
					(length 2.54)
					(name "D1_N")
					(number "11")
				)
				(pin bidirectional line
					(at 40.64 -6.35 180)
					(length 2.54)
					(name "D1_P")
					(number "12")
				)
				(pin output line
					(at 40.64 -19.05 180)
					(length 2.54)
					(name "~{PWRON2}")
					(number "13")
				)
				(pin input line
					(at 40.64 -16.51 180)
					(length 2.54)
					(name "~{OVRCUR2}")
					(number "14")
				)
				(pin bidirectional line
					(at 40.64 -24.13 180)
					(length 2.54)
					(name "D2_N")
					(number "15")
				)
				(pin bidirectional line
					(at 40.64 -21.59 180)
					(length 2.54)
					(name "D2_P")
					(number "16")
				)
				(pin output line
					(at 40.64 -34.29 180)
					(length 2.54)
					(name "~{PWRON3}")
					(number "17")
				)
				(pin input line
					(at 40.64 -31.75 180)
					(length 2.54)
					(name "~{OVRCUR3}")
					(number "18")
				)
				(pin bidirectional line
					(at 40.64 -39.37 180)
					(length 2.54)
					(name "D3_N")
					(number "19")
				)
				(pin bidirectional line
					(at 40.64 -36.83 180)
					(length 2.54)
					(name "D3_P")
					(number "20")
				)
				(pin output line
					(at 40.64 -49.53 180)
					(length 2.54)
					(name "~{PWRON4}")
					(number "21")
				)
				(pin input line
					(at 40.64 -46.99 180)
					(length 2.54)
					(name "~{OVRCUR4}")
					(number "22")
				)
				(pin bidirectional line
					(at 40.64 -54.61 180)
					(length 2.54)
					(name "D4_N")
					(number "23")
				)
				(pin bidirectional line
					(at 40.64 -52.07 180)
					(length 2.54)
					(name "D4_P")
					(number "24")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "25")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "~{EXTMEM}")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 2.54)
					(name "TSTPLL")
					(number "27")
					(alternate "48MCLK" passive line)
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "28")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 2.54)
					(name "XTAL2")
					(number "29")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "XTAL1")
					(number "30")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "TSTMODE")
					(number "31")
				)
				(pin output line
					(at 0 -11.43 0)
					(length 2.54)
					(name "SUSPND")
					(number "32")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "EP")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
