(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TUSB2077APTR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 58.42 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TUSB2077APTR"
				(at 58.42 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TUSB2077APTR"
				(at 58.42 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tusb2077a.pdf?ts=1702488653074&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FTUSB2077A"
				(at 58.42 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "7-Port Hub USB 2.0 LQFP-48"
				(at 58.42 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TUSB2077APTR"
				(at 58.42 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 58.42 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 58.42 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 58.42 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TUSB2077APTR_1_1"
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "SUSPND")
					(number "1")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DP0PUR")
					(number "2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "DP0")
					(number "3")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 2.54)
					(name "DM0")
					(number "4")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{RESET}")
					(number "6")
				)
				(pin passive clock
					(at 0 -73.66 0)
					(length 2.54)
					(name "EECLK")
					(number "7")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "EEDATA/~GANGED")
					(number "8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "9")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{BUSPWR}")
					(number "10")
				)
				(pin passive line
					(at 45.72 -73.66 180)
					(length 2.54)
					(name "~{PWRON1}")
					(number "11")
				)
				(pin passive line
					(at 45.72 -53.34 180)
					(length 2.54)
					(name "~{OVRCUR1}")
					(number "12")
				)
				(pin passive line
					(at 45.72 -2.54 180)
					(length 2.54)
					(name "DM1")
					(number "13")
				)
				(pin passive line
					(at 45.72 0 180)
					(length 2.54)
					(name "DP1")
					(number "14")
				)
				(pin passive line
					(at 45.72 -76.2 180)
					(length 2.54)
					(name "~{PWRON2}")
					(number "15")
				)
				(pin passive line
					(at 45.72 -55.88 180)
					(length 2.54)
					(name "~{OVRCUR2}")
					(number "16")
				)
				(pin passive line
					(at 45.72 -10.16 180)
					(length 2.54)
					(name "DM2")
					(number "17")
				)
				(pin passive line
					(at 45.72 -7.62 180)
					(length 2.54)
					(name "DP2")
					(number "18")
				)
				(pin passive line
					(at 45.72 -78.74 180)
					(length 2.54)
					(name "~{PWRON3}")
					(number "19")
				)
				(pin passive line
					(at 45.72 -58.42 180)
					(length 2.54)
					(name "~{OVRCUR3}")
					(number "20")
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 2.54)
					(name "DM3")
					(number "21")
				)
				(pin passive line
					(at 45.72 -15.24 180)
					(length 2.54)
					(name "DP3")
					(number "22")
				)
				(pin passive line
					(at 45.72 -81.28 180)
					(length 2.54)
					(name "~{PWRON4}")
					(number "23")
				)
				(pin power_in line
					(at 0 -88.9 0)
					(length 2.54)
					(name "GND")
					(number "24")
				)
				(pin passive line
					(at 45.72 -60.96 180)
					(length 2.54)
					(name "~{OVRCUR4}")
					(number "25")
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 2.54)
					(name "DM4")
					(number "26")
				)
				(pin passive line
					(at 45.72 -22.86 180)
					(length 2.54)
					(name "DP4")
					(number "27")
				)
				(pin passive line
					(at 45.72 -83.82 180)
					(length 2.54)
					(name "~{PWRON5}")
					(number "28")
				)
				(pin passive line
					(at 45.72 -63.5 180)
					(length 2.54)
					(name "~{OVRCUR5}")
					(number "29")
				)
				(pin passive line
					(at 45.72 -33.02 180)
					(length 2.54)
					(name "DM5")
					(number "30")
				)
				(pin passive line
					(at 45.72 -30.48 180)
					(length 2.54)
					(name "DP5")
					(number "31")
				)
				(pin passive line
					(at 45.72 -86.36 180)
					(length 2.54)
					(name "~{PWRON6}")
					(number "32")
				)
				(pin passive line
					(at 45.72 -66.04 180)
					(length 2.54)
					(name "~{OVRCUR6}")
					(number "33")
				)
				(pin passive line
					(at 45.72 -40.64 180)
					(length 2.54)
					(name "DM6")
					(number "34")
				)
				(pin passive line
					(at 45.72 -38.1 180)
					(length 2.54)
					(name "DP6")
					(number "35")
				)
				(pin passive line
					(at 45.72 -88.9 180)
					(length 2.54)
					(name "~{PWRON7}")
					(number "36")
				)
				(pin passive line
					(at 45.72 -68.58 180)
					(length 2.54)
					(name "~{OVRCUR7}")
					(number "37")
				)
				(pin passive line
					(at 45.72 -45.72 180)
					(length 2.54)
					(name "DM7")
					(number "38")
				)
				(pin passive line
					(at 45.72 -48.26 180)
					(length 2.54)
					(name "DP7")
					(number "39")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "HUBCFG")
					(number "40")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "PORTPWR")
					(number "41")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "PORTDIS")
					(number "42")
				)
				(pin passive line
					(at 0 -88.9 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "43")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "XTAL2")
					(number "44")
				)
				(pin passive clock
					(at 0 -40.64 0)
					(length 2.54)
					(name "XTAL1/CLK48")
					(number "45")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "46")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{EXTMEM}")
					(number "47")
				)
				(pin passive line
					(at 0 -86.36 0)
					(length 2.54)
					(name "MODE")
					(number "48")
				)
			)
			(embedded_fonts no)
		)
)
