(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TUSB8041IPAPRQ1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 76.2 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TUSB8041IPAPRQ1"
				(at 76.2 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TUSB8041IPAPRQ1"
				(at 76.2 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.ti.com/lit/gpn/TUSB8041-Q1"
				(at 76.2 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Automotive Four-Port SuperSpeed 5.0Gbps USB 3.0 Hub"
				(at 76.2 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TUSB8041IPAPRQ1"
				(at 76.2 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 76.2 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 76.2 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 76.2 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, ETHERNET, PHY,USB"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TUSB8041IPAPRQ1_1_1"
				(text "HOST"
					(at 23.495 -54.61 900)
				)
				(text "PORT1"
					(at 38.735 -12.7 900)
				)
				(text "PORT2"
					(at 38.735 -40.64 900)
				)
				(text "PORT3"
					(at 38.735 -68.58 900)
				)
				(text "PORT4"
					(at 38.735 -96.52 900)
				)
				(pin passive line
					(at 60.96 -55.88 180)
					(length 2.54)
					(name "PWRCTL3/BATEN3")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD33")
					(number "2")
				)
				(pin passive line
					(at 60.96 -27.94 180)
					(length 2.54)
					(name "PWRCTL2/BATEN2")
					(number "3")
				)
				(pin passive line
					(at 60.96 0 180)
					(length 2.54)
					(name "PWRCTL1/BATEN1")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "SDA/SMBDAT")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "SCL/SMBCLK")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 2.54)
					(name "SMBUSz/SS_SUSPEND")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 2.54)
					(name "FULLPWRMGMTZ/SMBA1/SS_UP")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 2.54)
					(name "PWRCTL_POL")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 2.54)
					(name "GANGED/SMBAS2/HS_UP")
					(number "10")
				)
				(pin passive line
					(at 60.96 -86.36 180)
					(length 2.54)
					(name "OVERCUR4z")
					(number "11")
				)
				(pin passive line
					(at 60.96 -58.42 180)
					(length 2.54)
					(name "OVERCUR3z")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 2.54)
					(name "AUTOENZ/HS_SUSPEND")
					(number "13")
				)
				(pin passive line
					(at 60.96 -2.54 180)
					(length 2.54)
					(name "OVERCUR1z")
					(number "14")
				)
				(pin passive line
					(at 60.96 -30.48 180)
					(length 2.54)
					(name "OVERCUR2z")
					(number "15")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "USB_VBUS")
					(number "16")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "TEST")
					(number "17")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "~{GRSTz}")
					(number "18")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "19")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD33")
					(number "20")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "USB_DP_UP")
					(number "21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "USB_DM_UP")
					(number "22")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "USB_SSTXP_UP")
					(number "23")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "USB_SSTXM_UP")
					(number "24")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "25")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "USB_SSRXP_UP")
					(number "26")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "USB_SSRXM_UP")
					(number "27")
				)
				(pin no_connect line
					(at 2.54 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "28")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(name "XO")
					(number "29")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "XI")
					(number "30")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD33")
					(number "31")
				)
				(pin input line
					(at 0 -99.06 0)
					(length 2.54)
					(name "USB_R1")
					(number "32")
				)
				(pin passive line
					(at 60.96 -17.78 180)
					(length 2.54)
					(name "USB_DP_DN1")
					(number "33")
				)
				(pin passive line
					(at 60.96 -20.32 180)
					(length 2.54)
					(name "USB_DM_DN1")
					(number "34")
				)
				(pin passive line
					(at 60.96 -7.62 180)
					(length 2.54)
					(name "USB_SSTXP_DN1")
					(number "35")
				)
				(pin passive line
					(at 60.96 -10.16 180)
					(length 2.54)
					(name "USB_SSTXM_DN1")
					(number "36")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "37")
				)
				(pin passive line
					(at 60.96 -12.7 180)
					(length 2.54)
					(name "USB_SSRXP_DN1")
					(number "38")
				)
				(pin passive line
					(at 60.96 -15.24 180)
					(length 2.54)
					(name "USB_SSRXM_DN1")
					(number "39")
				)
				(pin no_connect line
					(at 2.54 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "40")
				)
				(pin passive line
					(at 60.96 -45.72 180)
					(length 2.54)
					(name "USB_DP_DN2")
					(number "41")
				)
				(pin passive line
					(at 60.96 -48.26 180)
					(length 2.54)
					(name "USB_DM_DN2")
					(number "42")
				)
				(pin passive line
					(at 60.96 -35.56 180)
					(length 2.54)
					(name "USB_SSTXP_DN2")
					(number "43")
				)
				(pin passive line
					(at 60.96 -38.1 180)
					(length 2.54)
					(name "USB_SSTXM_DN2")
					(number "44")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "45")
				)
				(pin passive line
					(at 60.96 -40.64 180)
					(length 2.54)
					(name "USB_SSRXP_DN2")
					(number "46")
				)
				(pin passive line
					(at 60.96 -43.18 180)
					(length 2.54)
					(name "USB_SSRXM_DN2")
					(number "47")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD33")
					(number "48")
				)
				(pin passive line
					(at 60.96 -73.66 180)
					(length 2.54)
					(name "USB_DP_DN3")
					(number "49")
				)
				(pin passive line
					(at 60.96 -76.2 180)
					(length 2.54)
					(name "USB_DM_DN3")
					(number "50")
				)
				(pin passive line
					(at 60.96 -63.5 180)
					(length 2.54)
					(name "USB_SSTXP_DN3")
					(number "51")
				)
				(pin passive line
					(at 60.96 -66.04 180)
					(length 2.54)
					(name "USB_SSTXM_DN3")
					(number "52")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "53")
				)
				(pin passive line
					(at 60.96 -68.58 180)
					(length 2.54)
					(name "USB_SSRXP_DN3")
					(number "54")
				)
				(pin passive line
					(at 60.96 -71.12 180)
					(length 2.54)
					(name "USB_SSRXM_DN3")
					(number "55")
				)
				(pin passive line
					(at 60.96 -101.6 180)
					(length 2.54)
					(name "USB_DP_DN4")
					(number "56")
				)
				(pin passive line
					(at 60.96 -104.14 180)
					(length 2.54)
					(name "USB_DM_DN4")
					(number "57")
				)
				(pin passive line
					(at 60.96 -91.44 180)
					(length 2.54)
					(name "USB_SSTXP_DN4")
					(number "58")
				)
				(pin passive line
					(at 60.96 -93.98 180)
					(length 2.54)
					(name "USB_SSTXM_DN4")
					(number "59")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "60")
				)
				(pin passive line
					(at 60.96 -96.52 180)
					(length 2.54)
					(name "USB_SSRXP_DN4")
					(number "61")
				)
				(pin passive line
					(at 60.96 -99.06 180)
					(length 2.54)
					(name "USB_SSRXM_DN4")
					(number "62")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "63")
				)
				(pin passive line
					(at 60.96 -83.82 180)
					(length 2.54)
					(name "PWRCTL4/BATEN4")
					(number "64")
				)
				(pin power_in line
					(at 0 -104.14 0)
					(length 2.54)
					(name "GND")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
