(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "TUSB9261IPVP"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "TUSB9261IPVP"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "TUSB9261IPVP"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.ti.com/lit/gpn/tusb9261"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB 3.0 5 Gbps to SATA Bridge"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "TUSB9261IPVP"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Texas Instruments"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, USB, SATA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "TUSB9261IPVP_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "1")
				)
				(pin output line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "PWM0")
					(number "2")
				)
				(pin output line
					(at 30.48 -45.72 180)
					(length 2.54)
					(name "PWM1")
					(number "3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "GRSTz")
					(number "4")
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "GPIO8")
					(number "5")
					(alternate "UART_RX" passive line)
				)
				(pin bidirectional line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "GPIO9")
					(number "6")
					(alternate "UART_TX" passive line)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD33")
					(number "7")
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 2.54)
					(name "GPIO0")
					(number "8")
				)
				(pin bidirectional line
					(at 30.48 -15.24 180)
					(length 2.54)
					(name "GPIO1")
					(number "9")
				)
				(pin bidirectional line
					(at 30.48 -17.78 180)
					(length 2.54)
					(name "GPIO2")
					(number "10")
				)
				(pin bidirectional line
					(at 30.48 -20.32 180)
					(length 2.54)
					(name "GPIO3")
					(number "11")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "12")
				)
				(pin bidirectional line
					(at 30.48 -22.86 180)
					(length 2.54)
					(name "GPIO4")
					(number "13")
				)
				(pin bidirectional line
					(at 30.48 -25.4 180)
					(length 2.54)
					(name "GPIO5")
					(number "14")
				)
				(pin bidirectional line
					(at 30.48 -27.94 180)
					(length 2.54)
					(name "GPIO6")
					(number "15")
				)
				(pin bidirectional line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "GPIO7")
					(number "16")
				)
				(pin output line
					(at 30.48 -50.8 180)
					(length 2.54)
					(name "SPI_SCLK")
					(number "17")
				)
				(pin output line
					(at 30.48 -53.34 180)
					(length 2.54)
					(name "SPI_DATA_OUT")
					(number "18")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "19")
				)
				(pin input line
					(at 30.48 -55.88 180)
					(length 2.54)
					(name "SPI_DATA_IN")
					(number "20")
				)
				(pin output line
					(at 30.48 -58.42 180)
					(length 2.54)
					(name "SPI_CS0")
					(number "21")
				)
				(pin output line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "SPI_CS1")
					(number "22")
					(alternate "GPIO10" bidirectional line)
				)
				(pin output line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "SPI_CS2")
					(number "23")
					(alternate "GPIO11" bidirectional line)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD33")
					(number "24")
				)
				(pin input line
					(at 30.48 -63.5 180)
					(length 2.54)
					(name "JTAG_TCK")
					(number "25")
				)
				(pin input line
					(at 30.48 -66.04 180)
					(length 2.54)
					(name "JTAG_TDI")
					(number "26")
				)
				(pin output line
					(at 30.48 -68.58 180)
					(length 2.54)
					(name "JTAG_TDO")
					(number "27")
				)
				(pin input line
					(at 30.48 -71.12 180)
					(length 2.54)
					(name "JTAG_TMS")
					(number "28")
				)
				(pin input line
					(at 30.48 -73.66 180)
					(length 2.54)
					(name "JTAG_TRSTz")
					(number "29")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "FREQSEL0")
					(number "30")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "FREQSEL1")
					(number "31")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "32")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "33")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDA33")
					(number "34")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "USB_D-")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "USB_D+")
					(number "36")
				)
				(pin no_connect line
					(at 2.54 -50.8 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "37")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "USB_R1")
					(number "38")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(name "USB_R1RTN")
					(number "39")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDDA33")
					(number "40")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "41")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 2.54)
					(name "USB_SSTX-")
					(number "42")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 2.54)
					(name "USB_SSTX+")
					(number "43")
				)
				(pin power_in line
					(at 0 -73.66 0)
					(length 2.54)
					(name "VSS")
					(number "44")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 2.54)
					(name "USB_SSRX-")
					(number "45")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "USB_SSRX+")
					(number "46")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "47")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDDA33")
					(number "48")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "49")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "USB_VBUS")
					(number "50")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD33")
					(number "51")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "XI")
					(number "52")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 2.54)
					(name "VSSOSC")
					(number "53")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 2.54)
					(name "XO")
					(number "54")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "55")
				)
				(pin output line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "SATA_TX-")
					(number "56")
				)
				(pin output line
					(at 30.48 0 180)
					(length 2.54)
					(name "SATA_TX+")
					(number "57")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "58")
				)
				(pin input line
					(at 30.48 -7.62 180)
					(length 2.54)
					(name "SATA_RX-")
					(number "59")
				)
				(pin input line
					(at 30.48 -5.08 180)
					(length 2.54)
					(name "SATA_RX+")
					(number "60")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "61")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDDA33")
					(number "62")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "63")
				)
				(pin no_connect line
					(at 2.54 -53.34 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "64")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
