(footprint "Conn_Amphenol_SFP28_Cage_U773GC16382071"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -8.625 -13.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Conn_Amphenol_SFP28_Cage_U773GC16382071"
		(at -9.137 45.1 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at -2 49 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 7.123 30.001 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -9.137 46.3 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -9.137 47.5 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -9.137 48.7 0)
		(layer "F.Fab")
	)
	(fp_text user "LED location"
		(at 9.48 -11.445 0)
		(layer "User.1")
	)
	(fp_text user "PCB Edge"
		(at 9.48 35.055 0)
		(layer "User.1")
	)
	(fp_text user "Max hight 1.5mm"
		(at -22.02 -9.195 0)
		(unlocked yes)
		(layer "User.2")
	)
	(fp_text user "Max hight 1.5mm"
		(at 8.98 -9.195 0)
		(unlocked yes)
		(layer "User.2")
	)
	(fp_text user "Max hight 5mm"
		(at -6.12 -13.695 0)
		(unlocked yes)
		(layer "User.3")
	)
	(fp_text user ""
		(at -0.002 30.901 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at -0.002 30.901 0)
		(layer "User.9")
	)
	(pad "" np_thru_hole circle
		(at -7.125 -1.6)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -7.125 3.4)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -7.125 8.1)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at -4.8 -6.2)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 0 -6.2)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 4.8 -6.2)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.125 -1.6)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.125 3.4)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "" np_thru_hole circle
		(at 7.125 8.1)
		(size 0.95 0.95)
		(drill 0.95)
		(layers "*.Cu" "*.Mask")
	)
	(pad "SH" thru_hole rect
		(at -7.125 0.9)
		(size 2 2)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "SH" thru_hole rect
		(at -7.125 10.9)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "SH" thru_hole rect
		(at -7.125 20.9)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "SH" thru_hole rect
		(at -7.125 30.9)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "SH" smd rect
		(at 0 12.9)
		(size 12.05 2)
		(layers "F.Cu" "F.Paste")
	)
	(pad "SH" thru_hole rect
		(at 7.125 -4.1)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "SH" thru_hole rect
		(at 7.125 5.9)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "SH" thru_hole rect
		(at 7.125 15.9)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(pad "SH" thru_hole rect
		(at 7.125 25.9)
		(size 2 2)
		(drill 1.1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.102)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -1.747 -6.899) (xy 1.353 -6.899) (xy 1.353 -5.899) (xy -1.747 -5.899)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 8.123 4.901) (xy 8.123 -3.099) (xy 6.123 -3.099) (xy 6.123 4.901)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -8.127 -0.099) (xy -8.127 -6.899) (xy -3.447 -6.899) (xy -3.447 -5.899) (xy -6.127 -5.899) (xy -6.127 -0.099)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 8.123 -5.099) (xy 8.123 -6.899) (xy 3.053 -6.899) (xy 3.053 -5.899) (xy 6.123 -5.899) (xy 6.123 -5.099)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.01)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 8.123 35.401) (xy -8.127 35.401) (xy -8.127 31.901) (xy -6.127 31.901) (xy -6.127 29.901) (xy -8.127 29.901)
				(xy -8.127 21.901) (xy -6.127 21.901) (xy -6.127 19.901) (xy -8.127 19.901) (xy -8.127 11.901) (xy -6.127 11.901)
				(xy -6.127 9.901) (xy -8.127 9.901) (xy -8.127 1.901) (xy -6.127 1.901) (xy -6.127 8.601) (xy 6.123 8.601)
				(xy 6.123 6.901) (xy 8.123 6.901) (xy 8.123 14.901) (xy 6.123 14.901) (xy 6.123 16.901) (xy 8.123 16.901)
				(xy 8.123 24.901) (xy 6.123 24.901) (xy 6.123 26.901) (xy 8.123 26.901)
			)
		)
	)
	(embedded_fonts no)
	(model "antmicro_u773gc16382071.glb"
		(offset
			(xyz -15.48 29.905 -24.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 -0 -0)
		)
	)
)
