(footprint "USB-A_Receptacle_Amphenol_UE27AC54100"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -5.12 -1.85 0)
		(layer "F.SilkS")
	)
	(property "Value" "USB-A_Receptacle_Amphenol_UE27AC54100"
		(at -5.12 14.51 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 3.5 2.71 0)
		(layer "F.Fab")
	)
	(property "Description" ""
		(at 3.5 2.71 0)
		(layer "F.Fab")
	)
	(attr through_hole)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "In1.Cu")
		(layer "In2.Cu")
		(layer "In3.Cu")
		(layer "In4.Cu")
		(layer "In5.Cu")
		(layer "In6.Cu")
		(layer "In7.Cu")
		(layer "In8.Cu")
		(layer "In9.Cu")
		(layer "In10.Cu")
		(layer "In11.Cu")
		(layer "In12.Cu")
		(layer "In13.Cu")
		(layer "In14.Cu")
		(layer "In15.Cu")
		(layer "In16.Cu")
		(layer "In17.Cu")
		(layer "In18.Cu")
		(layer "User.1")
		(layer "In19.Cu")
		(layer "User.2")
		(layer "In20.Cu")
		(layer "User.3")
		(layer "In21.Cu")
		(layer "User.4")
		(layer "In22.Cu")
		(layer "User.5")
		(layer "In23.Cu")
		(layer "User.6")
		(layer "In24.Cu")
		(layer "User.7")
		(layer "In25.Cu")
		(layer "User.8")
		(layer "In26.Cu")
		(layer "User.9")
		(layer "In27.Cu")
		(layer "In28.Cu")
		(layer "In29.Cu")
		(layer "In30.Cu")
		(layer "In31.Cu")
		(layer "In32.Cu")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.12 15.71 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.12 16.91 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.12 18.11 0)
		(layer "F.Fab")
	)
	(fp_text user ""
		(at 3.5 2.71 0)
		(layer "User.5")
	)
	(fp_text user ""
		(at 3.5 2.71 0)
		(layer "User.9")
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.8 1.8)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole circle
		(at 2.5 0)
		(size 1.8 1.8)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole circle
		(at 4.5 0)
		(size 1.8 1.8)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 7 0)
		(size 1.8 1.8)
		(drill 0.92)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at -3.07 2.71)
		(size 3.3 3.3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "SH" thru_hole circle
		(at 10.07 2.71)
		(size 3.3 3.3)
		(drill 2.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "antmicro_ue27ac54100.glb"
		(offset
			(xyz 3.5 0.79 6.87)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
