(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "Amphenol_SFP28_1x20_UE763GA202600T"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "J"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "Amphenol_SFP28_1x20_UE763GA202600T"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "Amphenol_SFP28_1x20_UE763GA202600T"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://cdn.amphenol-cs.com/media/wysiwyg/files/documentation/datasheet/inputoutput/hsio_cn_ultraport_sfp.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "20 Position SFP28 Receptacle with no Cage, Right Angle"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "UE763GA202600T"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Amphenol"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "CONNECTOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "Amphenol_SFP28_1x20_UE763GA202600T_1_1"
				(text "SFP28\n"
					(at 16.51 0 0)
				)
				(pin passive line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "V_{EE}(T)")
					(number "1")
				)
				(pin open_collector line
					(at 0 -20.32 0)
					(length 2.54)
					(name "TX_{FAULT}")
					(number "2")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "TX_{DISABLE}")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SDA")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SCL")
					(number "5")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "MOD_{ABS}")
					(number "6")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "RS0")
					(number "7")
				)
				(pin open_collector line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RX_{LOS}")
					(number "8")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RS1")
					(number "9")
				)
				(pin passive line
					(at 25.4 -43.18 180)
					(length 2.54)
					(name "V_{EE}(R)")
					(number "10")
				)
				(pin passive line
					(at 25.4 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "V_{EE}(R)")
					(number "11")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 2.54)
					(name "RD-")
					(number "12")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 2.54)
					(name "RD+")
					(number "13")
				)
				(pin passive line
					(at 25.4 -43.18 180)
					(length 2.54)
					(hide yes)
					(name "V_{EE}(R)")
					(number "14")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}(R)")
					(number "15")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "V_{CC}(T)")
					(number "16")
				)
				(pin passive line
					(at 25.4 -40.64 180)
					(length 2.54)
					(hide yes)
					(name "V_{EE}(T)")
					(number "17")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "TD+")
					(number "18")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "TD-")
					(number "19")
				)
				(pin passive line
					(at 25.4 -40.64 180)
					(length 2.54)
					(hide yes)
					(name "V_{EE}(T)")
					(number "20")
				)
			)
			(embedded_fonts no)
		)
)
