(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB1T1105AMHX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB1T1105AMHX"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB1T1105AMHX"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/usb1t1105a-d.pdf"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Transceiver with voltage regulator"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "USB1T1105AMHX"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Onsemi"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "USB, IC, TRANSCEIVER, REGULATOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB1T1105AMHX_1_1"
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "~{OE}")
					(number "1")
				)
				(pin output line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "RCV")
					(number "2")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VP")
					(number "3")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 2.54)
					(name "VM")
					(number "4")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "SUSPND")
					(number "5")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "MODE")
					(number "6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCCIO")
					(number "7")
				)
				(pin no_connect line
					(at 22.86 -22.86 180)
					(length 2.54)
					(name "NC")
					(number "8")
				)
				(pin passive line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "D-")
					(number "9")
				)
				(pin passive line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "D+")
					(number "10")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VPO/VO")
					(number "11")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VMO/FSEO")
					(number "12")
				)
				(pin passive line
					(at 25.4 -6.35 180)
					(length 2.54)
					(name "VREG_3P3")
					(number "13")
				)
				(pin power_in line
					(at 25.4 0 180)
					(length 2.54)
					(name "VCC_5P0")
					(number "14")
				)
				(pin passive line
					(at 25.4 -3.81 180)
					(length 2.54)
					(name "VPU_3P3")
					(number "15")
				)
				(pin passive line
					(at 25.4 -16.51 180)
					(length 2.54)
					(name "CONFIG")
					(number "16")
				)
				(pin passive line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "EPAD")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
