(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB2412"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB2412"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB2412"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/2412.pdf"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface, USB Hub Controller, USB 2.0, 3 V, 3.6 V, QFN, 28 Pins"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "USB2412-DZK"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB2412_1_1"
				(text "PORT 1"
					(at 18.415 -12.065 0)
				)
				(text "PORT 2"
					(at 18.415 -26.035 0)
				)
				(pin bidirectional line
					(at 33.02 -6.35 180)
					(length 2.54)
					(name "DN1_D+")
					(number "1")
				)
				(pin bidirectional line
					(at 33.02 -22.86 180)
					(length 2.54)
					(name "DN2_D-")
					(number "2")
				)
				(pin bidirectional line
					(at 33.02 -20.32 180)
					(length 2.54)
					(name "DN2_D+")
					(number "3")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "3V3")
					(number "4")
				)
				(pin no_connect line
					(at 0 -17.78 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 0 -20.32 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin output line
					(at 33.02 0 180)
					(length 2.54)
					(name "PWR_{PRT1}")
					(number "7")
				)
				(pin input line
					(at 33.02 -2.54 180)
					(length 2.54)
					(name "OCS_{N1}")
					(number "8")
				)
				(pin passive line
					(at 33.02 -29.21 180)
					(length 2.54)
					(name "CRFILT")
					(number "9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "3V3")
					(number "10")
				)
				(pin output line
					(at 33.02 -13.97 180)
					(length 2.54)
					(name "PWR_{PRT2}")
					(number "11")
				)
				(pin input line
					(at 33.02 -16.51 180)
					(length 2.54)
					(name "OCS_{N2}")
					(number "12")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 2.54)
					(name "NON_REM1")
					(number "13")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "3V3")
					(number "14")
				)
				(pin passive line
					(at 33.02 -36.83 180)
					(length 2.54)
					(name "TEST1")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "HS_{IND}")
					(number "16")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{RESET}")
					(number "17")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "VBUS_{DET}")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "SUSP_{IND}/NON_REM0")
					(number "19")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "3V3")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "UP_D-")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "UP_D+")
					(number "22")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "XTAL_{OUT}")
					(number "23")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "XTAL_{IN}")
					(number "24")
				)
				(pin passive line
					(at 33.02 -31.75 180)
					(length 2.54)
					(name "PLLFILT")
					(number "25")
				)
				(pin passive line
					(at 33.02 -34.29 180)
					(length 2.54)
					(name "R_{BIAS}")
					(number "26")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "3V3")
					(number "27")
				)
				(pin bidirectional line
					(at 33.02 -8.89 180)
					(length 2.54)
					(name "DN1_D-")
					(number "28")
				)
				(pin passive line
					(at 33.02 -40.64 180)
					(length 2.54)
					(name "EP")
					(number "29")
				)
			)
			(embedded_fonts no)
		)
)
