(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB2514B-I_M2"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 60.96 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB2514B-I_M2"
				(at 60.96 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB2514B-I_M2"
				(at 60.96 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/00001692C.pdf"
				(at 60.96 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface, USB Hub Controller, USB 2.0, 3 V, 3.6 V, QFN, 36 Pins"
				(at 60.96 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 60.96 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "USB2514BI-AEZG"
				(at 60.96 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 60.96 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 60.96 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB2514B-I_M2_0_0")
			(symbol "USB2514B-I_M2_1_1"
				(text "PORT 1"
					(at 32.385 -14.605 0)
				)
				(text "PORT 2"
					(at 32.385 -29.845 0)
				)
				(text "PORT 3"
					(at 32.385 -45.085 0)
				)
				(text "PORT 4"
					(at 32.385 -60.325 0)
				)
				(pin bidirectional line
					(at 50.8 -12.7 180)
					(length 2.54)
					(name "DN1_D-")
					(number "1")
				)
				(pin bidirectional line
					(at 50.8 -10.16 180)
					(length 2.54)
					(name "DN1_D+")
					(number "2")
				)
				(pin bidirectional line
					(at 50.8 -27.94 180)
					(length 2.54)
					(name "DN2_D-")
					(number "3")
				)
				(pin bidirectional line
					(at 50.8 -25.4 180)
					(length 2.54)
					(name "DN2_D+")
					(number "4")
				)
				(pin passive line
					(at 12.7 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDDA33")
					(number "5")
				)
				(pin bidirectional line
					(at 50.8 -43.18 180)
					(length 2.54)
					(name "DN3_D-")
					(number "6")
				)
				(pin bidirectional line
					(at 50.8 -40.64 180)
					(length 2.54)
					(name "DN3_D+")
					(number "7")
				)
				(pin bidirectional line
					(at 50.8 -58.42 180)
					(length 2.54)
					(name "DN4_D-")
					(number "8")
				)
				(pin bidirectional line
					(at 50.8 -55.88 180)
					(length 2.54)
					(name "DN4_D+")
					(number "9")
				)
				(pin power_in line
					(at 12.7 -5.08 0)
					(length 2.54)
					(name "VDDA33")
					(number "10")
				)
				(pin input line
					(at 50.8 -63.5 180)
					(length 2.54)
					(name "TEST")
					(number "11")
				)
				(pin input line
					(at 50.8 -2.54 180)
					(length 2.54)
					(name "PWR_{PRT1}/BC_{EN1}")
					(number "12")
				)
				(pin input line
					(at 50.8 -5.08 180)
					(length 2.54)
					(name "OCS_{N1}")
					(number "13")
				)
				(pin passive line
					(at 50.8 -68.58 180)
					(length 2.54)
					(name "CRFILT")
					(number "14")
				)
				(pin power_in line
					(at 12.7 -2.54 0)
					(length 2.54)
					(name "VDD33")
					(number "15")
				)
				(pin input line
					(at 50.8 -17.78 180)
					(length 2.54)
					(name "PWR_{PRT2}/BC_{EN2}")
					(number "16")
				)
				(pin input line
					(at 50.8 -20.32 180)
					(length 2.54)
					(name "OCS_{N2}")
					(number "17")
				)
				(pin input line
					(at 50.8 -33.02 180)
					(length 2.54)
					(name "PWR_{PRT3}/BC_{EN3}")
					(number "18")
				)
				(pin input line
					(at 50.8 -35.56 180)
					(length 2.54)
					(name "OCS_{N3}")
					(number "19")
				)
				(pin input line
					(at 50.8 -48.26 180)
					(length 2.54)
					(name "PWR_{PRT4}/BC_{EN4}")
					(number "20")
				)
				(pin input line
					(at 50.8 -50.8 180)
					(length 2.54)
					(name "OCS_{N4}")
					(number "21")
				)
				(pin bidirectional line
					(at 12.7 -66.04 0)
					(length 2.54)
					(name "SMBDATA/NON_REM1")
					(number "22")
				)
				(pin passive line
					(at 12.7 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD33")
					(number "23")
				)
				(pin input line
					(at 12.7 -68.58 0)
					(length 2.54)
					(name "SMBCLK/CFG_SEL0")
					(number "24")
				)
				(pin input line
					(at 12.7 -71.12 0)
					(length 2.54)
					(name "HS_IND/CFG_SEL1")
					(number "25")
				)
				(pin input line
					(at 12.7 -15.24 0)
					(length 2.54)
					(name "~{RESET}")
					(number "26")
				)
				(pin input line
					(at 12.7 -20.32 0)
					(length 2.54)
					(name "VBUS_{DET}")
					(number "27")
				)
				(pin bidirectional line
					(at 12.7 -63.5 0)
					(length 2.54)
					(name "SUSP_IND/NON_REM0")
					(number "28")
				)
				(pin passive line
					(at 12.7 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDDA33")
					(number "29")
				)
				(pin bidirectional line
					(at 12.7 -27.94 0)
					(length 2.54)
					(name "UP_D-")
					(number "30")
				)
				(pin bidirectional line
					(at 12.7 -25.4 0)
					(length 2.54)
					(name "UP_D+")
					(number "31")
				)
				(pin output line
					(at 12.7 -45.72 0)
					(length 2.54)
					(name "XTAL_{OUT}")
					(number "32")
				)
				(pin input line
					(at 12.7 -33.02 0)
					(length 2.54)
					(name "XTAL_{IN}")
					(number "33")
				)
				(pin passive line
					(at 50.8 -71.12 180)
					(length 2.54)
					(name "PLLFILT")
					(number "34")
				)
				(pin bidirectional line
					(at 50.8 -73.66 180)
					(length 2.54)
					(name "R_{BIAS}")
					(number "35")
				)
				(pin passive line
					(at 12.7 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDDA33")
					(number "36")
				)
				(pin power_in line
					(at 12.7 -73.66 0)
					(length 2.54)
					(name "VSS")
					(number "37")
				)
			)
			(embedded_fonts no)
		)
)
