(footprint "QFN-48-1EP_7x7x0.9mm_P0.5mm_EP5x5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -5.202 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-48-1EP_7x7x0.9mm_P0.5mm_EP5x5mm"
		(at -10.55 5.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "."
		(at -4.4 -3.05 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at -4.202 7.2 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.202 8.4 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.202 9.598 0)
		(layer "F.Fab")
	)
	(pad "1" smd oval
		(at -3.5 -2.75 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -3.5 -2.25 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -3.5 -1.75 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -3.5 -1.25 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -3.5 -0.75 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -3.5 -0.25 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -3.5 0.248 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -3.5 0.748 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -3.5 1.249 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -3.5 1.749 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -3.5 2.249 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -3.5 2.749 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at -2.75 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at -2.25 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at -1.75 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at -1.25 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at -0.75 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at -0.25 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at 0.248 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at 0.748 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at 1.249 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at 1.749 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at 2.249 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at 2.749 3.499)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at 3.499 2.749 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 3.499 2.249 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 3.499 1.749 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 3.499 1.249 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at 3.499 0.748 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at 3.499 0.248 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 3.499 -0.25 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 3.499 -0.75 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at 3.499 -1.25 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at 3.499 -1.75 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at 3.499 -2.25 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd oval
		(at 3.499 -2.75 90)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd oval
		(at 2.749 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd oval
		(at 2.249 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd oval
		(at 1.749 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd oval
		(at 1.249 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd oval
		(at 0.748 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd oval
		(at 0.248 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd oval
		(at -0.25 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd oval
		(at -0.75 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd oval
		(at -1.25 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd oval
		(at -1.75 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd oval
		(at -2.25 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd oval
		(at -2.75 -3.5)
		(size 0.3 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 0 0)
		(size 5 5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_usb2642_ml.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
