(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB2642_ML"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 76.2 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB2642_ML"
				(at 76.2 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB2642_ML"
				(at 76.2 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/00001578D.pdf"
				(at 76.2 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface, USB Hub and Flash Media Controller, USB 2.0, 3 V, 3.6 V, QFN, 48 Pins"
				(at 76.2 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "USB2642/ML"
				(at 76.2 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 76.2 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 76.2 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 76.2 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "USB, HUB, INTERFACE, CONTROLLER, FLASH "
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB2642_ML_1_1"
				(pin passive line
					(at 49.53 -12.7 180)
					(length 2.54)
					(name "USBDN_DM2")
					(number "1")
				)
				(pin passive line
					(at 49.53 -10.16 180)
					(length 2.54)
					(name "USBDN_DP2")
					(number "2")
				)
				(pin passive line
					(at 49.53 -26.67 180)
					(length 2.54)
					(name "USBDN_DM3")
					(number "3")
				)
				(pin passive line
					(at 49.53 -24.13 180)
					(length 2.54)
					(name "USBDN_DP3")
					(number "4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDA33_1")
					(number "5")
				)
				(pin passive line
					(at 49.53 -7.62 180)
					(length 2.54)
					(name "PRTCTL2")
					(number "6")
				)
				(pin passive line
					(at 49.53 -21.59 180)
					(length 2.54)
					(name "PRTCTL3")
					(number "7")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 2.54)
					(name "SPI_CE_N")
					(number "8")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 2.54)
					(name "SPI_CLK/SCL_EP")
					(number "9")
				)
				(pin passive line
					(at 0 -67.31 0)
					(length 2.54)
					(name "SPI_DO/SDA_EP/SPI_SPD_SEL")
					(number "10")
				)
				(pin passive line
					(at 0 -69.85 0)
					(length 2.54)
					(name "SPI_DI")
					(number "11")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VDD33_1")
					(number "12")
				)
				(pin passive line
					(at 49.53 -33.02 180)
					(length 2.54)
					(name "SD_WP")
					(number "13")
				)
				(pin passive line
					(at 49.53 -36.83 180)
					(length 2.54)
					(name "SD_NCD")
					(number "14")
				)
				(pin passive line
					(at 0 -80.01 0)
					(length 2.54)
					(name "VDD18")
					(number "15")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD33_2")
					(number "16")
				)
				(pin passive line
					(at 49.53 -57.15 180)
					(length 2.54)
					(name "SD_D1")
					(number "17")
				)
				(pin passive line
					(at 49.53 -54.61 180)
					(length 2.54)
					(name "SD_D0")
					(number "18")
				)
				(pin passive line
					(at 49.53 -72.39 180)
					(length 2.54)
					(name "SD_D7")
					(number "19")
				)
				(pin passive line
					(at 49.53 -69.85 180)
					(length 2.54)
					(name "SD_D6")
					(number "20")
				)
				(pin passive line
					(at 49.53 -74.93 180)
					(length 2.54)
					(name "SD_CLK")
					(number "21")
				)
				(pin passive line
					(at 0 -77.47 0)
					(length 2.54)
					(name "REG_EN")
					(number "22")
				)
				(pin passive line
					(at 49.53 -67.31 180)
					(length 2.54)
					(name "SD_D5")
					(number "23")
				)
				(pin passive line
					(at 49.53 -44.45 180)
					(length 2.54)
					(name "SD_CMD")
					(number "24")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD33_3")
					(number "25")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD33_(OTP)")
					(number "26")
				)
				(pin passive line
					(at 0 -97.79 0)
					(length 2.54)
					(hide yes)
					(name "TEST1")
					(number "27")
				)
				(pin passive line
					(at 0 -97.79 0)
					(length 2.54)
					(hide yes)
					(name "TEST2")
					(number "28")
				)
				(pin passive line
					(at 0 -52.07 0)
					(length 2.54)
					(name "SDA")
					(number "29")
				)
				(pin passive line
					(at 49.53 -64.77 180)
					(length 2.54)
					(name "SD_D4")
					(number "30")
				)
				(pin no_connect line
					(at 46.99 -81.28 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "31")
				)
				(pin passive line
					(at 49.53 -62.23 180)
					(length 2.54)
					(name "SD_D3")
					(number "32")
				)
				(pin passive line
					(at 49.53 -59.69 180)
					(length 2.54)
					(name "SD_D2")
					(number "33")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD33_4")
					(number "34")
				)
				(pin passive line
					(at 49.53 -40.64 180)
					(length 2.54)
					(name "CRD_PWR")
					(number "35")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 2.54)
					(name "SCL")
					(number "36")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 2.54)
					(name "GPO1")
					(number "37")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(name "RESET_N")
					(number "38")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VBUS_DET")
					(number "39")
				)
				(pin passive line
					(at 0 -97.79 0)
					(length 2.54)
					(name "TEST0")
					(number "40")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDDA33_2")
					(number "41")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 2.54)
					(name "USBUP_DP")
					(number "42")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "USBUP_DM")
					(number "43")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "XTAL2")
					(number "44")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 2.54)
					(name "XTAL1_(CLKIN)")
					(number "45")
				)
				(pin passive line
					(at 0 -82.55 0)
					(length 2.54)
					(name "VDD18PLL")
					(number "46")
				)
				(pin passive line
					(at 0 -92.71 0)
					(length 2.54)
					(name "RBIAS")
					(number "47")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDDA33_3")
					(number "48")
				)
				(pin passive line
					(at 0 -100.33 0)
					(length 2.54)
					(name "VSS")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
