(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB3300-EZK-TR"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB3300-EZK-TR"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB3300-EZK-TR"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/00001783C.pdf"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface, USB Host Controller, USB 2.0 OTG, 3 V, 3.6 V, VQFN, 32 Pins"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "USB3300-EZK-TR"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, CONTROLLER, IC, USB, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB3300-EZK-TR_0_0"
				(pin power_in line
					(at 0 -43.18 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "2")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 2.54)
					(name "CPEN")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VBUS")
					(number "4")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "ID")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD3.3")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DP")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DM")
					(number "8")
				)
				(pin input line
					(at 24.13 -40.64 180)
					(length 2.54)
					(name "RESET")
					(number "9")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "EXTVBUS")
					(number "10")
				)
				(pin output line
					(at 24.13 -30.48 180)
					(length 2.54)
					(name "NXT")
					(number "11")
				)
				(pin output line
					(at 24.13 -33.02 180)
					(length 2.54)
					(name "DIR")
					(number "12")
				)
				(pin input line
					(at 24.13 -35.56 180)
					(length 2.54)
					(name "STP")
					(number "13")
				)
				(pin output clock
					(at 24.13 -38.1 180)
					(length 2.54)
					(name "CLKOUT")
					(number "14")
				)
				(pin power_in line
					(at 24.13 0 180)
					(length 2.54)
					(name "VDD1.8")
					(number "15")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD3.3")
					(number "16")
				)
				(pin bidirectional line
					(at 24.13 -25.4 180)
					(length 2.54)
					(name "DATA[7]")
					(number "17")
				)
				(pin bidirectional line
					(at 24.13 -22.86 180)
					(length 2.54)
					(name "DATA[6]")
					(number "18")
				)
				(pin bidirectional line
					(at 24.13 -20.32 180)
					(length 2.54)
					(name "DATA[5]")
					(number "19")
				)
				(pin bidirectional line
					(at 24.13 -17.78 180)
					(length 2.54)
					(name "DATA[4]")
					(number "20")
				)
				(pin bidirectional line
					(at 24.13 -15.24 180)
					(length 2.54)
					(name "DATA[3]")
					(number "21")
				)
				(pin bidirectional line
					(at 24.13 -12.7 180)
					(length 2.54)
					(name "DATA[2]")
					(number "22")
				)
				(pin bidirectional line
					(at 24.13 -10.16 180)
					(length 2.54)
					(name "DATA[1]")
					(number "23")
				)
				(pin bidirectional line
					(at 24.13 -7.62 180)
					(length 2.54)
					(name "DATA[0]")
					(number "24")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD3.3")
					(number "25")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 2.54)
					(hide yes)
					(name "VDD1.8")
					(number "26")
				)
				(pin output line
					(at 0 -34.29 0)
					(length 2.54)
					(name "XO")
					(number "27")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "XI")
					(number "28")
				)
				(pin power_in line
					(at 24.13 -2.54 180)
					(length 2.54)
					(name "VDDA1.8")
					(number "29")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD3.3")
					(number "30")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "REG_EN")
					(number "31")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "RBIAS")
					(number "32")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "EP")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
