(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB3340-EZK-TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB3340-EZK-TR"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB3340-EZK-TR"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/268/MCHP_S_A0010410418_1-2552239.pdf"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface, USB PHY Transceiver, USB 2.0, 3 V, 5.5 V, QFN, 32 Pins"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "USB3340-EZK-TR"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, USB, INTERFACE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB3340-EZK-TR_1_1"
				(pin output line
					(at 30.48 -43.18 180)
					(length 2.54)
					(name "CLKOUT")
					(number "1")
				)
				(pin output line
					(at 30.48 -38.1 180)
					(length 2.54)
					(name "NXT")
					(number "2")
				)
				(pin bidirectional line
					(at 30.48 -8.89 180)
					(length 2.54)
					(name "DATA0")
					(number "3")
				)
				(pin bidirectional line
					(at 30.48 -11.43 180)
					(length 2.54)
					(name "DATA1")
					(number "4")
				)
				(pin bidirectional line
					(at 30.48 -13.97 180)
					(length 2.54)
					(name "DATA2")
					(number "5")
				)
				(pin bidirectional line
					(at 30.48 -16.51 180)
					(length 2.54)
					(name "DATA3")
					(number "6")
				)
				(pin bidirectional line
					(at 30.48 -19.05 180)
					(length 2.54)
					(name "DATA4")
					(number "7")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "REFSEL0")
					(number "8")
				)
				(pin bidirectional line
					(at 30.48 -21.59 180)
					(length 2.54)
					(name "DATA5")
					(number "9")
				)
				(pin bidirectional line
					(at 30.48 -24.13 180)
					(length 2.54)
					(name "DATA6")
					(number "10")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "REFSEL1")
					(number "11")
				)
				(pin no_connect line
					(at 0 -16.51 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin bidirectional line
					(at 30.48 -26.67 180)
					(length 2.54)
					(name "DATA7")
					(number "13")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "REFSEL2")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "SPK_L")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "SPK_R")
					(number "16")
				)
				(pin output line
					(at 30.48 -30.48 180)
					(length 2.54)
					(name "CPEN")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "D_P")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "D_N")
					(number "19")
				)
				(pin power_out line
					(at 30.48 0 180)
					(length 2.54)
					(name "VDD33")
					(number "20")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VBAT")
					(number "21")
				)
				(pin bidirectional line
					(at 30.48 -33.02 180)
					(length 2.54)
					(name "VBUS")
					(number "22")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "ID")
					(number "23")
				)
				(pin passive line
					(at 30.48 -6.35 180)
					(length 2.54)
					(name "RBIAS")
					(number "24")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "XO")
					(number "25")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "REFCLK")
					(number "26")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "RESETB")
					(number "27")
				)
				(pin power_out line
					(at 30.48 -2.54 180)
					(length 2.54)
					(name "VDD18")
					(number "28")
				)
				(pin input line
					(at 30.48 -35.56 180)
					(length 2.54)
					(name "STP")
					(number "29")
				)
				(pin no_connect line
					(at 0 -13.97 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "30")
				)
				(pin output line
					(at 30.48 -40.64 180)
					(length 2.54)
					(name "DIR")
					(number "31")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDIO")
					(number "32")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 2.54)
					(name "GND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
