(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB5742_2G"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 81.28 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB5742_2G"
				(at 81.28 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB5742_2G"
				(at 81.28 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/UNG/ProductDocuments/DataSheets/USB5742B-Data-Sheet-DS00002016.pdf"
				(at 81.28 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB Interface, USB Hub Controller, USB 2.0/3.0, 3-3.6 V, SQFN, 56 Pins"
				(at 81.28 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "USB5742B/2G"
				(at 81.28 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 81.28 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 81.28 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 81.28 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, USB, HUB"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB5742_2G_0_0"
				(text "UP PORT"
					(at 19.685 -44.45 0)
				)
				(text "PORT 1"
					(at 30.48 -20.32 0)
				)
				(text "PORT 2"
					(at 30.48 -44.45 0)
				)
			)
			(symbol "USB5742_2G_0_1")
			(symbol "USB5742_2G_1_1"
				(pin bidirectional line
					(at 50.8 -3.81 180)
					(length 2.54)
					(name "DN1_D+/DIS")
					(number "1")
				)
				(pin bidirectional line
					(at 50.8 -6.35 180)
					(length 2.54)
					(name "DN1_D-/DIS")
					(number "2")
				)
				(pin bidirectional line
					(at 50.8 -16.51 180)
					(length 2.54)
					(name "DN1_SSTX+")
					(number "3")
				)
				(pin bidirectional line
					(at 50.8 -19.05 180)
					(length 2.54)
					(name "DN1_SSTX-")
					(number "4")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "VDD12")
					(number "5")
				)
				(pin bidirectional line
					(at 50.8 -10.16 180)
					(length 2.54)
					(name "DN1_SSRX+")
					(number "6")
				)
				(pin bidirectional line
					(at 50.8 -12.7 180)
					(length 2.54)
					(name "DN1_SSRX-")
					(number "7")
				)
				(pin bidirectional line
					(at 50.8 -27.94 180)
					(length 2.54)
					(name "DN2_D+/DIS")
					(number "8")
				)
				(pin bidirectional line
					(at 50.8 -30.48 180)
					(length 2.54)
					(name "DN2_D-/DIS")
					(number "9")
				)
				(pin bidirectional line
					(at 50.8 -40.64 180)
					(length 2.54)
					(name "DN2_SSTX+")
					(number "10")
				)
				(pin bidirectional line
					(at 50.8 -43.18 180)
					(length 2.54)
					(name "DN2_SSTX-")
					(number "11")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD12")
					(number "12")
				)
				(pin bidirectional line
					(at 50.8 -34.29 180)
					(length 2.54)
					(name "DN2_SSRX+")
					(number "13")
				)
				(pin bidirectional line
					(at 50.8 -36.83 180)
					(length 2.54)
					(name "DN2_SSRX-")
					(number "14")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "VDD12")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD33")
					(number "16")
				)
				(pin no_connect line
					(at 48.26 -52.07 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "17")
				)
				(pin no_connect line
					(at 48.26 -53.34 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "18")
				)
				(pin no_connect line
					(at 48.26 -54.61 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "19")
				)
				(pin no_connect line
					(at 48.26 -55.88 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "20")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "VDD12")
					(number "21")
				)
				(pin no_connect line
					(at 48.26 -57.15 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "22")
				)
				(pin no_connect line
					(at 48.26 -58.42 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "23")
				)
				(pin no_connect line
					(at 48.26 -59.69 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "24")
				)
				(pin no_connect line
					(at 48.26 -60.96 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "25")
				)
				(pin no_connect line
					(at 48.26 -62.23 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "26")
				)
				(pin no_connect line
					(at 48.26 -63.5 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "27")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "VDD12")
					(number "28")
				)
				(pin no_connect line
					(at 48.26 -64.77 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "29")
				)
				(pin no_connect line
					(at 48.26 -66.04 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "30")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD33")
					(number "31")
				)
				(pin bidirectional line
					(at 50.8 -72.39 180)
					(length 2.54)
					(name "GANG_PWR/GPIO20")
					(number "32")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "VDD12")
					(number "33")
				)
				(pin bidirectional line
					(at 50.8 -48.26 180)
					(length 2.54)
					(name "GPIO19")
					(number "34")
				)
				(pin bidirectional line
					(at 50.8 -24.13 180)
					(length 2.54)
					(name "PRT_CTL2")
					(number "35")
				)
				(pin bidirectional line
					(at 50.8 0 180)
					(length 2.54)
					(name "PRT_CTL1")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 2.54)
					(name "VBUS_DET/GPIO16")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "SPI_CLK/SMCLK")
					(number "38")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "SPI_DO/SMDAT")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "SPI_DI/CFG_BC_EN")
					(number "40")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "SPI_CE_N/CFG_NON_REM")
					(number "41")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RESET_N")
					(number "42")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "VDD12")
					(number "43")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD33")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "UP_D+")
					(number "45")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "UP_D-")
					(number "46")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "UP_SSTX+")
					(number "47")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "UP_SSTX-")
					(number "48")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "VDD12")
					(number "49")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "UP_SSRX+")
					(number "50")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "UP_SSRX-")
					(number "51")
				)
				(pin input line
					(at 0 -80.01 0)
					(length 2.54)
					(name "ATEST")
					(number "52")
				)
				(pin output line
					(at 0 -62.23 0)
					(length 2.54)
					(name "XTALO")
					(number "53")
				)
				(pin input line
					(at 0 -49.53 0)
					(length 2.54)
					(name "XTALI/CLK_IN")
					(number "54")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD33")
					(number "55")
				)
				(pin input line
					(at 0 -82.55 0)
					(length 2.54)
					(name "RBIAS")
					(number "56")
				)
				(pin power_in line
					(at 0 -91.44 0)
					(length 2.54)
					(name "VSS")
					(number "57")
				)
			)
			(embedded_fonts no)
		)
)
