(footprint "QFN-56-1EP_7x7mm_P0.4mm_EP4.6x4.6mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "QFN 56 Pin")
	(tags "QFN")
	(property "Reference" "REF**"
		(at -4.05 -3.88 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-56-1EP_7x7mm_P0.4mm_EP4.6x4.6mm"
		(at -4.06 4.84 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -4.06 6.84 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.06 8.04 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.06 9.24 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.525 -1.525)
		(size 1.3 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at -1.525 0)
		(size 1.3 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at -1.525 1.525)
		(size 1.3 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 0 -1.525)
		(size 1.3 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.3 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 0 1.525)
		(size 1.3 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 1.525 -1.525)
		(size 1.3 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 1.525 0)
		(size 1.3 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "" smd roundrect
		(at 1.525 1.525)
		(size 1.3 1.3)
		(layers "F.Paste")
		(roundrect_rratio 0.221239)
	)
	(pad "1" smd oval
		(at -3.4 -2.6)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd oval
		(at -3.4 -2.2)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd oval
		(at -3.4 -1.8)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd oval
		(at -3.4 -1.4)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd oval
		(at -3.4 -1)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd oval
		(at -3.4 -0.6)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd oval
		(at -3.4 -0.2)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd oval
		(at -3.4 0.2)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd oval
		(at -3.4 0.6)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd oval
		(at -3.4 1)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd oval
		(at -3.4 1.4)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd oval
		(at -3.4 1.8)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd oval
		(at -3.4 2.2)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd oval
		(at -3.4 2.6)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd oval
		(at -2.6 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd oval
		(at -2.2 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd oval
		(at -1.8 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd oval
		(at -1.4 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd oval
		(at -1 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd oval
		(at -0.6 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd oval
		(at -0.2 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd oval
		(at 0.2 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd oval
		(at 0.6 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd oval
		(at 1 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd oval
		(at 1.4 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd oval
		(at 1.8 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd oval
		(at 2.2 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd oval
		(at 2.6 3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd oval
		(at 3.4 2.6)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd oval
		(at 3.4 2.2)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd oval
		(at 3.4 1.8)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd oval
		(at 3.4 1.4)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd oval
		(at 3.4 1)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd oval
		(at 3.4 0.6)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd oval
		(at 3.4 0.2)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd oval
		(at 3.4 -0.2)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd oval
		(at 3.4 -0.6)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd oval
		(at 3.4 -1)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd oval
		(at 3.4 -1.4)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd oval
		(at 3.4 -1.8)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd oval
		(at 3.4 -2.2)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd oval
		(at 3.4 -2.6)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd oval
		(at 2.6 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd oval
		(at 2.2 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd oval
		(at 1.8 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd oval
		(at 1.4 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd oval
		(at 1 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd oval
		(at 0.6 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd oval
		(at 0.2 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "50" smd oval
		(at -0.2 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "51" smd oval
		(at -0.6 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "52" smd oval
		(at -1 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "53" smd oval
		(at -1.4 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "54" smd oval
		(at -1.8 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "55" smd oval
		(at -2.2 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "56" smd oval
		(at -2.6 -3.4 90)
		(size 0.8 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "57" smd rect
		(at 0 0)
		(size 4.6 4.6)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_usb5744_i_2g.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
