(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB7016_KDX"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 71.12 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB7016_KDX"
				(at 71.12 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB7016_KDX"
				(at 71.12 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/USB7016-Data-Sheet-DS00003740B.pdf"
				(at 71.12 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "USB hub controller"
				(at 71.12 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "USB7016/KDX"
				(at 71.12 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 71.12 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 71.12 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 71.12 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, CONTROLLER, IC, USB, HUB, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "VQFN100_KDX_MCH VQFN100_KDX_MCH-M VQFN100_KDX_MCH-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB7016_KDX_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "RESET_N")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 3.81)
					(name "PF30")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 3.81)
					(name "PF31")
					(number "3")
				)
				(pin bidirectional line
					(at 49.53 -5.08 180)
					(length 3.81)
					(name "DP1_VBUS_MON")
					(number "4")
				)
				(pin bidirectional line
					(at 49.53 -35.56 180)
					(length 3.81)
					(name "USB2DN_DP1/PRT_DIS_P1")
					(number "5")
				)
				(pin bidirectional line
					(at 49.53 -38.1 180)
					(length 3.81)
					(name "USB2DN_DM1/PRT_DIS_M1")
					(number "6")
				)
				(pin bidirectional line
					(at 49.53 -15.24 180)
					(length 3.81)
					(name "USB3DN_TXDP1A")
					(number "7")
				)
				(pin bidirectional line
					(at 49.53 -17.78 180)
					(length 3.81)
					(name "USB3DN_TXDM1A")
					(number "8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "9")
				)
				(pin bidirectional line
					(at 49.53 -20.32 180)
					(length 3.81)
					(name "USB3DN_RXDP1A")
					(number "10")
				)
				(pin bidirectional line
					(at 49.53 -22.86 180)
					(length 3.81)
					(name "USB3DN_RXDM1A")
					(number "11")
				)
				(pin bidirectional line
					(at 49.53 -10.16 180)
					(length 3.81)
					(name "DP1_CC1")
					(number "12")
				)
				(pin bidirectional line
					(at 49.53 -12.7 180)
					(length 3.81)
					(name "DP1_CC2")
					(number "13")
				)
				(pin bidirectional line
					(at 49.53 -96.52 180)
					(length 3.81)
					(name "USB2DN_DP5/PRT_DIS_P5")
					(number "14")
				)
				(pin bidirectional line
					(at 49.53 -99.06 180)
					(length 3.81)
					(name "USB2DN_DM5/PRT_DIS_M5")
					(number "15")
				)
				(pin bidirectional line
					(at 49.53 -25.4 180)
					(length 3.81)
					(name "USB3DN_TXDP1B")
					(number "16")
				)
				(pin bidirectional line
					(at 49.53 -27.94 180)
					(length 3.81)
					(name "USB3DN_TXDM1B")
					(number "17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCORE")
					(number "18")
				)
				(pin bidirectional line
					(at 49.53 -30.48 180)
					(length 3.81)
					(name "USB3DN_RXDP1B")
					(number "19")
				)
				(pin bidirectional line
					(at 49.53 -33.02 180)
					(length 3.81)
					(name "USB3DN_RXDM1B")
					(number "20")
				)
				(pin input line
					(at 0 -99.06 0)
					(length 3.81)
					(name "CFG_STRAP1")
					(number "21")
				)
				(pin input line
					(at 0 -101.6 0)
					(length 3.81)
					(name "CFG_STRAP2")
					(number "22")
				)
				(pin input line
					(at 0 -104.14 0)
					(length 3.81)
					(name "CFG_STRAP3")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 3.81)
					(name "TESTEN")
					(number "24")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "25")
				)
				(pin power_in line
					(at 49.53 0 180)
					(length 3.81)
					(name "VDD33")
					(number "26")
				)
				(pin bidirectional line
					(at 49.53 -53.34 180)
					(length 3.81)
					(name "USB2DN_DP2/PRT_DIS_P2")
					(number "27")
				)
				(pin bidirectional line
					(at 49.53 -55.88 180)
					(length 3.81)
					(name "USB2DN_DM2/PRT_DIS_M2")
					(number "28")
				)
				(pin bidirectional line
					(at 49.53 -43.18 180)
					(length 3.81)
					(name "USB3DN_TXDP2")
					(number "29")
				)
				(pin bidirectional line
					(at 49.53 -45.72 180)
					(length 3.81)
					(name "USB3DN_TXDM2")
					(number "30")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "31")
				)
				(pin bidirectional line
					(at 49.53 -48.26 180)
					(length 3.81)
					(name "USB3DN_RXDP2")
					(number "32")
				)
				(pin bidirectional line
					(at 49.53 -50.8 180)
					(length 3.81)
					(name "USB3DN_RXDM2")
					(number "33")
				)
				(pin bidirectional line
					(at 49.53 -71.12 180)
					(length 3.81)
					(name "USB2DN_DP3/PRT_DIS_P3")
					(number "34")
				)
				(pin bidirectional line
					(at 49.53 -73.66 180)
					(length 3.81)
					(name "USB2DN_DM3/PRT_DIS_M3")
					(number "35")
				)
				(pin bidirectional line
					(at 49.53 -60.96 180)
					(length 3.81)
					(name "USB3DN_TXDP3")
					(number "36")
				)
				(pin bidirectional line
					(at 49.53 -63.5 180)
					(length 3.81)
					(name "USB3DN_TXDM3")
					(number "37")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "38")
				)
				(pin bidirectional line
					(at 49.53 -66.04 180)
					(length 3.81)
					(name "USB3DN_RXDP3")
					(number "39")
				)
				(pin bidirectional line
					(at 49.53 -68.58 180)
					(length 3.81)
					(name "USB3DN_RXDM3")
					(number "40")
				)
				(pin bidirectional line
					(at 49.53 -106.68 180)
					(length 3.81)
					(name "USB2DN_DM6/PRT_DIS_M6")
					(number "41")
				)
				(pin bidirectional line
					(at 49.53 -104.14 180)
					(length 3.81)
					(name "USB2DN_DP6/PRT_DIS_P6")
					(number "42")
				)
				(pin passive line
					(at 49.53 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PF3")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PF4")
					(number "45")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PF5")
					(number "46")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PF6")
					(number "47")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PF7")
					(number "48")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PF8")
					(number "49")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PF9")
					(number "50")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PF10")
					(number "51")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PF11")
					(number "52")
				)
				(pin passive line
					(at 49.53 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PF12")
					(number "54")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "55")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PF13")
					(number "56")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PF14")
					(number "57")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PF15")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PF16")
					(number "59")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PF17")
					(number "60")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PF18")
					(number "61")
				)
				(pin passive line
					(at 49.53 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "62")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 3.81)
					(name "TEST1")
					(number "63")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 3.81)
					(name "TEST2")
					(number "64")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 3.81)
					(name "TEST3")
					(number "65")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PF19")
					(number "66")
				)
				(pin passive line
					(at 49.53 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "67")
				)
				(pin bidirectional line
					(at 49.53 -111.76 180)
					(length 3.81)
					(name "SPI_CLK/PF21")
					(number "68")
				)
				(pin bidirectional line
					(at 49.53 -114.3 180)
					(length 3.81)
					(name "SPI_CE_N/CFG_NON_REM/PF20")
					(number "69")
				)
				(pin bidirectional line
					(at 49.53 -116.84 180)
					(length 3.81)
					(name "SPI_D0/CFG_BC_EN/PF22")
					(number "70")
				)
				(pin bidirectional line
					(at 49.53 -119.38 180)
					(length 3.81)
					(name "SPI_D1/PF23")
					(number "71")
				)
				(pin bidirectional line
					(at 49.53 -121.92 180)
					(length 3.81)
					(name "SPI_D2/PF24")
					(number "72")
				)
				(pin bidirectional line
					(at 49.53 -124.46 180)
					(length 3.81)
					(name "SPI_D3/PF25")
					(number "73")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 3.81)
					(name "PF29")
					(number "74")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "PF26")
					(number "75")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "PF27")
					(number "76")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 3.81)
					(name "PF28")
					(number "77")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "78")
				)
				(pin passive line
					(at 49.53 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "79")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VBUS_MON_UP")
					(number "80")
				)
				(pin bidirectional line
					(at 49.53 -88.9 180)
					(length 3.81)
					(name "USB2DN_DP4/PRT_DIS_P4")
					(number "81")
				)
				(pin bidirectional line
					(at 49.53 -91.44 180)
					(length 3.81)
					(name "USB2DN_DM4/PRT_DIS_M4")
					(number "82")
				)
				(pin bidirectional line
					(at 49.53 -78.74 180)
					(length 3.81)
					(name "USB3DN_TXDP4")
					(number "83")
				)
				(pin bidirectional line
					(at 49.53 -81.28 180)
					(length 3.81)
					(name "USB3DN_TXDM4")
					(number "84")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "85")
				)
				(pin bidirectional line
					(at 49.53 -83.82 180)
					(length 3.81)
					(name "USB3DN_RXDP4")
					(number "86")
				)
				(pin bidirectional line
					(at 49.53 -86.36 180)
					(length 3.81)
					(name "USB3DN_RXDM4")
					(number "87")
				)
				(pin passive line
					(at 49.53 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "88")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "USB2UP_DP")
					(number "89")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "USB2UP_DM")
					(number "90")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "USB3UP_TXDP")
					(number "91")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "USB3UP_TXDM")
					(number "92")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "93")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "USB3UP_RXDP")
					(number "94")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "USB3UP_RXDM")
					(number "95")
				)
				(pin no_connect line
					(at 3.81 -106.68 0)
					(length 3.81)
					(hide yes)
					(name "ATEST")
					(number "96")
				)
				(pin output line
					(at 0 -93.98 0)
					(length 3.81)
					(name "XTALO")
					(number "97")
				)
				(pin input line
					(at 0 -91.44 0)
					(length 3.81)
					(name "XTALI/CLK_IN")
					(number "98")
				)
				(pin passive line
					(at 49.53 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "99")
				)
				(pin input line
					(at 0 -121.92 0)
					(length 3.81)
					(name "RBIAS")
					(number "100")
				)
				(pin power_in line
					(at 0 -124.46 0)
					(length 3.81)
					(name "VSS")
					(number "101")
				)
			)
			(embedded_fonts no)
		)
)
