(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "USB7252C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 71.12 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "USB7252C"
				(at 71.12 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "USB7252C"
				(at 71.12 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/00003852A.pdf"
				(at 71.12 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "4-Port USB 3.2 Hub, 2x Type-C with Power Delivery support, 1x USB 3.2, 1x USB 2.0"
				(at 71.12 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "USB7252CT-I/KDX "
				(at 71.12 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 71.12 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 71.12 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 71.12 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "INTERFACE, CONTROLLER, IC, USB, HUB"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "USB7252C_1_1"
				(text "UP PORT"
					(at 16.51 -27.686 0)
				)
				(text "PORT 1\n"
					(at 30.226 -35.052 0)
				)
				(text "PORT 2\n"
					(at 30.226 -72.39 0)
				)
				(text "PORT 3\n"
					(at 30.226 -92.202 0)
				)
				(text "PORT 4\n"
					(at 30.226 -102.616 0)
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "RESET_N")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 3.81)
					(name "PF30")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 3.81)
					(name "PF31")
					(number "3")
				)
				(pin bidirectional line
					(at 55.88 -1.27 180)
					(length 3.81)
					(name "DP1_VBUS_MON")
					(number "4")
				)
				(pin bidirectional line
					(at 55.88 -29.21 180)
					(length 3.81)
					(name "USB2DN_DP1")
					(number "5")
					(alternate "PRT_DIS_P1" passive line)
				)
				(pin bidirectional line
					(at 55.88 -31.75 180)
					(length 3.81)
					(name "USB2DN_DM1")
					(number "6")
					(alternate "PRT_DIS_M1" passive line)
				)
				(pin bidirectional line
					(at 55.88 -13.97 180)
					(length 3.81)
					(name "USB3DN_TXDP1A")
					(number "7")
				)
				(pin bidirectional line
					(at 55.88 -16.51 180)
					(length 3.81)
					(name "USB3DN_TXDM1A")
					(number "8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "9")
				)
				(pin bidirectional line
					(at 55.88 -8.89 180)
					(length 3.81)
					(name "USB3DN_RXDP1A")
					(number "10")
				)
				(pin bidirectional line
					(at 55.88 -11.43 180)
					(length 3.81)
					(name "USB3DN_RXDM1A")
					(number "11")
				)
				(pin bidirectional line
					(at 55.88 -3.81 180)
					(length 3.81)
					(name "DP1_CC1")
					(number "12")
				)
				(pin bidirectional line
					(at 55.88 -6.35 180)
					(length 3.81)
					(name "DP1_CC2")
					(number "13")
				)
				(pin bidirectional line
					(at 55.88 -96.52 180)
					(length 3.81)
					(name "USB2DN_DP4")
					(number "14")
					(alternate "PRT_DIS_P4" passive line)
				)
				(pin bidirectional line
					(at 55.88 -99.06 180)
					(length 3.81)
					(name "USB2DN_DM4")
					(number "15")
					(alternate "PRT_DIS_M4" passive line)
				)
				(pin bidirectional line
					(at 55.88 -24.13 180)
					(length 3.81)
					(name "USB3DN_TXDP1B")
					(number "16")
				)
				(pin bidirectional line
					(at 55.88 -26.67 180)
					(length 3.81)
					(name "USB3DN_TXDM1B")
					(number "17")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCORE")
					(number "18")
				)
				(pin bidirectional line
					(at 55.88 -19.05 180)
					(length 3.81)
					(name "USB3DN_RXDP1B")
					(number "19")
				)
				(pin bidirectional line
					(at 55.88 -21.59 180)
					(length 3.81)
					(name "USB3DN_RXDM1B")
					(number "20")
				)
				(pin input line
					(at 0 -97.79 0)
					(length 3.81)
					(name "CFG_STRAP1")
					(number "21")
				)
				(pin input line
					(at 0 -100.33 0)
					(length 3.81)
					(name "CFG_STRAP2")
					(number "22")
				)
				(pin input line
					(at 0 -102.87 0)
					(length 3.81)
					(name "CFG_STRAP3")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 3.81)
					(name "TESTEN")
					(number "24")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "25")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDD33")
					(number "26")
				)
				(pin bidirectional line
					(at 55.88 -41.91 180)
					(length 3.81)
					(name "DP2_CC1")
					(number "27")
				)
				(pin bidirectional line
					(at 55.88 -44.45 180)
					(length 3.81)
					(name "DP2_CC2")
					(number "28")
				)
				(pin bidirectional line
					(at 55.88 -67.31 180)
					(length 3.81)
					(name "USB2DN_DP2")
					(number "29")
					(alternate "PRT_DIS_P2" passive line)
				)
				(pin bidirectional line
					(at 55.88 -69.85 180)
					(length 3.81)
					(name "USB2DN_DM2")
					(number "30")
					(alternate "PRT_DIS_M2" passive line)
				)
				(pin bidirectional line
					(at 55.88 -52.07 180)
					(length 3.81)
					(name "USB3DN_TXDP2A")
					(number "31")
				)
				(pin bidirectional line
					(at 55.88 -54.61 180)
					(length 3.81)
					(name "USB3DN_TXDM2A")
					(number "32")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "33")
				)
				(pin bidirectional line
					(at 55.88 -46.99 180)
					(length 3.81)
					(name "USB3DN_RXDP2A")
					(number "34")
				)
				(pin bidirectional line
					(at 55.88 -49.53 180)
					(length 3.81)
					(name "USB3DN_RXDM2A")
					(number "35")
				)
				(pin bidirectional line
					(at 55.88 -39.37 180)
					(length 3.81)
					(name "DP2_VBUS_MON")
					(number "36")
				)
				(pin bidirectional line
					(at 55.88 -62.23 180)
					(length 3.81)
					(name "USB3DN_TXDP2B")
					(number "37")
				)
				(pin bidirectional line
					(at 55.88 -64.77 180)
					(length 3.81)
					(name "USB3DN_TXDM2B")
					(number "38")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "39")
				)
				(pin bidirectional line
					(at 55.88 -57.15 180)
					(length 3.81)
					(name "USB3DN_RXDP2B")
					(number "40")
				)
				(pin bidirectional line
					(at 55.88 -59.69 180)
					(length 3.81)
					(name "USB3DN_RXDM2B")
					(number "41")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "42")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 3.81)
					(name "PF2")
					(number "43")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 3.81)
					(name "PF3")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 3.81)
					(name "PF4")
					(number "45")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 3.81)
					(name "PF5")
					(number "46")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 3.81)
					(name "PF6")
					(number "47")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 3.81)
					(name "PF7")
					(number "48")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 3.81)
					(name "PF8")
					(number "49")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 3.81)
					(name "PF9")
					(number "50")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 3.81)
					(name "PF10")
					(number "51")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 3.81)
					(name "PF11")
					(number "52")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 3.81)
					(name "PF12")
					(number "54")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "55")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 3.81)
					(name "PF13")
					(number "56")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 3.81)
					(name "PF14")
					(number "57")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 3.81)
					(name "PF15")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 3.81)
					(name "PF16")
					(number "59")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 3.81)
					(name "PF17")
					(number "60")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 3.81)
					(name "PF18")
					(number "61")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "62")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 3.81)
					(name "TEST1")
					(number "63")
				)
				(pin passive line
					(at 0 -111.76 0)
					(length 3.81)
					(name "TEST2")
					(number "64")
				)
				(pin passive line
					(at 0 -114.3 0)
					(length 3.81)
					(name "TEST3")
					(number "65")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 3.81)
					(name "PF19")
					(number "66")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "67")
				)
				(pin bidirectional line
					(at 55.88 -111.76 180)
					(length 3.81)
					(name "SPI_CLK")
					(number "68")
					(alternate "PF21" passive line)
				)
				(pin bidirectional line
					(at 55.88 -114.3 180)
					(length 3.81)
					(name "SPI_CE_N")
					(number "69")
					(alternate "CFG_NON_REM" passive line)
					(alternate "PF20" passive line)
				)
				(pin bidirectional line
					(at 55.88 -116.84 180)
					(length 3.81)
					(name "SPI_D0")
					(number "70")
					(alternate "CFG_BC_EN" passive line)
					(alternate "PF22" passive line)
				)
				(pin bidirectional line
					(at 55.88 -119.38 180)
					(length 3.81)
					(name "SPI_D1")
					(number "71")
					(alternate "PF23" passive line)
				)
				(pin bidirectional line
					(at 55.88 -121.92 180)
					(length 3.81)
					(name "SPI_D2")
					(number "72")
					(alternate "PF24" passive line)
				)
				(pin bidirectional line
					(at 55.88 -124.46 180)
					(length 3.81)
					(name "SPI_D3")
					(number "73")
					(alternate "PF25" passive line)
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 3.81)
					(name "PF29")
					(number "74")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 3.81)
					(name "PF26")
					(number "75")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 3.81)
					(name "PF27")
					(number "76")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 3.81)
					(name "PF28")
					(number "77")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "78")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "79")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VBUS_MON_UP")
					(number "80")
				)
				(pin bidirectional line
					(at 55.88 -86.36 180)
					(length 3.81)
					(name "USB2DN_DP3")
					(number "81")
					(alternate "PRT_DIS_P3" passive line)
				)
				(pin bidirectional line
					(at 55.88 -88.9 180)
					(length 3.81)
					(name "USB2DN_DM3")
					(number "82")
					(alternate "PRT_DIS_M3" passive line)
				)
				(pin bidirectional line
					(at 55.88 -76.2 180)
					(length 3.81)
					(name "USB3DN_TXDP3")
					(number "83")
				)
				(pin bidirectional line
					(at 55.88 -78.74 180)
					(length 3.81)
					(name "USB3DN_TXDM3")
					(number "84")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "85")
				)
				(pin bidirectional line
					(at 55.88 -81.28 180)
					(length 3.81)
					(name "USB3DN_RXDP3")
					(number "86")
				)
				(pin bidirectional line
					(at 55.88 -83.82 180)
					(length 3.81)
					(name "USB3DN_RXDM3")
					(number "87")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "88")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "USB2UP_DP")
					(number "89")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "USB2UP_DM")
					(number "90")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "USB3UP_TXDP")
					(number "91")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "USB3UP_TXDM")
					(number "92")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCORE")
					(number "93")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "USB3UP_RXDP")
					(number "94")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "USB3UP_RXDM")
					(number "95")
				)
				(pin no_connect line
					(at 3.81 -106.68 0)
					(length 3.81)
					(hide yes)
					(name "ATEST")
					(number "96")
				)
				(pin output line
					(at 0 -95.25 0)
					(length 3.81)
					(name "XTALO")
					(number "97")
				)
				(pin input line
					(at 0 -92.71 0)
					(length 3.81)
					(name "XTALI")
					(number "98")
					(alternate "CLK_IN" passive line)
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD33")
					(number "99")
				)
				(pin input line
					(at 0 -121.92 0)
					(length 3.81)
					(name "RBIAS")
					(number "100")
				)
				(pin power_in line
					(at 0 -124.46 0)
					(length 3.81)
					(name "VSS")
					(number "101")
				)
			)
			(embedded_fonts no)
		)
)
