(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "WiFi_WF121-A-V2"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "A"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "WiFi_WF121-A-V2"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "WiFi_WF121-A-V2"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/BlueGiga%20PDFs/WF121_Datasheet.pdf"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Wireless LAN Module, 2.4GHz, I2C, SPI, UART, USB, Navigation Devices, PoS Terminals, RFID, Cameras"
				(at 53.34 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "WF121-A-V2"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Silicon Labs"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MODULE, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "WiFi_WF121-A-V2_1_1"
				(pin power_in line
					(at 0 -63.5 0)
					(length 2.54)
					(name "GND")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 2.54)
					(name "RB15/CN12/AN15")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RE0")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RE1")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RE2")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RE3")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RE4")
					(number "7")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD_PA")
					(number "8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD_3.3V")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RE5")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "RE6")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "RE7")
					(number "12")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 2.54)
					(name "MCLR")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "RB1/CN3")
					(number "14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "RB0/CN2")
					(number "15")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "RB8")
					(number "17")
				)
				(pin bidirectional line
					(at 29.21 -5.08 180)
					(length 2.54)
					(name "RF3")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 2.54)
					(name "RB14")
					(number "19")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 2.54)
					(name "RB13")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "RB12")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 2.54)
					(name "RB11")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "RB10")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RB5/CN7")
					(number "24")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VBUS")
					(number "25")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "26")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 2.54)
					(name "RG3/D-")
					(number "27")
				)
				(pin input line
					(at 0 -58.42 0)
					(length 2.54)
					(name "RG2/D+")
					(number "28")
				)
				(pin bidirectional line
					(at 29.21 -7.62 180)
					(length 2.54)
					(name "RD3")
					(number "29")
				)
				(pin bidirectional line
					(at 29.21 -10.16 180)
					(length 2.54)
					(name "RC12")
					(number "30")
				)
				(pin bidirectional line
					(at 29.21 -12.7 180)
					(length 2.54)
					(name "RC15")
					(number "31")
				)
				(pin bidirectional line
					(at 29.21 -15.24 180)
					(length 2.54)
					(name "RD2")
					(number "32")
				)
				(pin bidirectional line
					(at 29.21 -17.78 180)
					(length 2.54)
					(name "RC13/CN1")
					(number "33")
				)
				(pin bidirectional line
					(at 29.21 -20.32 180)
					(length 2.54)
					(name "RC14/CN0")
					(number "34")
				)
				(pin bidirectional line
					(at 29.21 -22.86 180)
					(length 2.54)
					(name "RF4/CN17")
					(number "35")
				)
				(pin bidirectional line
					(at 29.21 -25.4 180)
					(length 2.54)
					(name "RF5/CN18")
					(number "36")
				)
				(pin bidirectional line
					(at 29.21 -27.94 180)
					(length 2.54)
					(name "RD11/INT4")
					(number "37")
				)
				(pin bidirectional line
					(at 29.21 -30.48 180)
					(length 2.54)
					(name "RD0/INT0")
					(number "38")
				)
				(pin bidirectional line
					(at 29.21 -33.02 180)
					(length 2.54)
					(name "RD4")
					(number "39")
				)
				(pin bidirectional line
					(at 29.21 0 180)
					(length 2.54)
					(name "BT_RF")
					(number "40")
				)
				(pin bidirectional line
					(at 29.21 -35.56 180)
					(length 2.54)
					(name "RD5")
					(number "41")
				)
				(pin bidirectional line
					(at 29.21 -38.1 180)
					(length 2.54)
					(name "RD6/CN15")
					(number "42")
				)
				(pin bidirectional line
					(at 29.21 -40.64 180)
					(length 2.54)
					(name "RD7/CN16")
					(number "43")
				)
				(pin bidirectional line
					(at 29.21 -43.18 180)
					(length 2.54)
					(name "RD9/INT2")
					(number "44")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "45")
				)
				(pin bidirectional line
					(at 29.21 -45.72 180)
					(length 2.54)
					(name "RD10/INT3")
					(number "46")
				)
				(pin bidirectional line
					(at 29.21 -48.26 180)
					(length 2.54)
					(name "RD1")
					(number "47")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "48")
				)
				(pin bidirectional line
					(at 29.21 -2.54 180)
					(length 2.54)
					(name "ANT")
					(number "49")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "50")
				)
				(pin power_in line
					(at 0 -60.96 0)
					(length 2.54)
					(name "GNDPAD")
					(number "51")
				)
				(pin unspecified line
					(at 29.21 -55.88 180)
					(length 2.54)
					(name "SPI_MISO")
					(number "52")
				)
				(pin unspecified line
					(at 29.21 -58.42 180)
					(length 2.54)
					(name "SPI_CLK")
					(number "53")
				)
				(pin unspecified line
					(at 29.21 -60.96 180)
					(length 2.54)
					(name "SPI_MOSI")
					(number "54")
				)
				(pin unspecified line
					(at 29.21 -63.5 180)
					(length 2.54)
					(name "SPI_CS")
					(number "55")
				)
			)
			(embedded_fonts no)
		)
)
